(kicad_pcb (version 20171130) (host pcbnew "(5.1.10)-1")

  (general
    (thickness 1.6)
    (drawings 0)
    (tracks 354)
    (zones 0)
    (modules 17)
    (nets 58)
  )

  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )

  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.1)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )

  (net 0 "")
  (net 1 GND)
  (net 2 "Net-(J1-Pad3)")
  (net 3 VCC)
  (net 4 "Net-(J1-Pad5)")
  (net 5 /SMI_SD13)
  (net 6 /I2S_SD)
  (net 7 /SEL_MODE3)
  (net 8 /SMI_SD8)
  (net 9 /I2S_WS)
  (net 10 /SMI_SD5)
  (net 11 /SMI_SD4)
  (net 12 /SEL_MODE2)
  (net 13 /SEL_MODE1)
  (net 14 /SMI_SD0)
  (net 15 /SMI_SD3)
  (net 16 /SMI_SD17)
  (net 17 /SMI_SD1)
  (net 18 /SMI_SD2)
  (net 19 /SMI_SD16)
  (net 20 +3V3)
  (net 21 /SMI_SD15)
  (net 22 /SMI_SD14)
  (net 23 /I2S_CLK)
  (net 24 /SMI_SD9)
  (net 25 /SMI_SD7)
  (net 26 /SMI_SD6)
  (net 27 +5V)
  (net 28 +12V)
  (net 29 "Net-(R3-Pad1)")
  (net 30 /SEL_MODE0)
  (net 31 "Net-(J1-Pad7)")
  (net 32 "Net-(J1-Pad13)")
  (net 33 "Net-(J1-Pad26)")
  (net 34 "Net-(J1-Pad27)")
  (net 35 "Net-(J1-Pad28)")
  (net 36 "Net-(J_OUT1-Pad1)")
  (net 37 "Net-(J_OUT1-Pad2)")
  (net 38 "Net-(J_OUT1-Pad3)")
  (net 39 "Net-(J_OUT1-Pad4)")
  (net 40 "Net-(J_OUT1-Pad5)")
  (net 41 "Net-(J_OUT1-Pad6)")
  (net 42 "Net-(J_OUT1-Pad7)")
  (net 43 "Net-(J_OUT1-Pad8)")
  (net 44 "Net-(J_OUT2-Pad1)")
  (net 45 "Net-(J_OUT2-Pad2)")
  (net 46 "Net-(J_OUT2-Pad3)")
  (net 47 "Net-(J_OUT2-Pad4)")
  (net 48 "Net-(J_OUT2-Pad5)")
  (net 49 "Net-(J_OUT2-Pad6)")
  (net 50 "Net-(J_OUT2-Pad7)")
  (net 51 "Net-(J_OUT2-Pad8)")
  (net 52 "Net-(OUT_5V1-Pad3)")
  (net 53 "Net-(OUT_5V1-Pad2)")
  (net 54 "Net-(OUT_5V1-Pad5)")
  (net 55 "Net-(R1-Pad1)")
  (net 56 "Net-(R2-Pad2)")
  (net 57 "Net-(U1-Pad9)")

  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +12V)
    (add_net +3V3)
    (add_net +5V)
    (add_net /I2S_CLK)
    (add_net /I2S_SD)
    (add_net /I2S_WS)
    (add_net /SEL_MODE0)
    (add_net /SEL_MODE1)
    (add_net /SEL_MODE2)
    (add_net /SEL_MODE3)
    (add_net /SMI_SD0)
    (add_net /SMI_SD1)
    (add_net /SMI_SD13)
    (add_net /SMI_SD14)
    (add_net /SMI_SD15)
    (add_net /SMI_SD16)
    (add_net /SMI_SD17)
    (add_net /SMI_SD2)
    (add_net /SMI_SD3)
    (add_net /SMI_SD4)
    (add_net /SMI_SD5)
    (add_net /SMI_SD6)
    (add_net /SMI_SD7)
    (add_net /SMI_SD8)
    (add_net /SMI_SD9)
    (add_net GND)
    (add_net "Net-(J1-Pad13)")
    (add_net "Net-(J1-Pad26)")
    (add_net "Net-(J1-Pad27)")
    (add_net "Net-(J1-Pad28)")
    (add_net "Net-(J1-Pad3)")
    (add_net "Net-(J1-Pad5)")
    (add_net "Net-(J1-Pad7)")
    (add_net "Net-(J_OUT1-Pad1)")
    (add_net "Net-(J_OUT1-Pad2)")
    (add_net "Net-(J_OUT1-Pad3)")
    (add_net "Net-(J_OUT1-Pad4)")
    (add_net "Net-(J_OUT1-Pad5)")
    (add_net "Net-(J_OUT1-Pad6)")
    (add_net "Net-(J_OUT1-Pad7)")
    (add_net "Net-(J_OUT1-Pad8)")
    (add_net "Net-(J_OUT2-Pad1)")
    (add_net "Net-(J_OUT2-Pad2)")
    (add_net "Net-(J_OUT2-Pad3)")
    (add_net "Net-(J_OUT2-Pad4)")
    (add_net "Net-(J_OUT2-Pad5)")
    (add_net "Net-(J_OUT2-Pad6)")
    (add_net "Net-(J_OUT2-Pad7)")
    (add_net "Net-(J_OUT2-Pad8)")
    (add_net "Net-(OUT_5V1-Pad2)")
    (add_net "Net-(OUT_5V1-Pad3)")
    (add_net "Net-(OUT_5V1-Pad5)")
    (add_net "Net-(R1-Pad1)")
    (add_net "Net-(R2-Pad2)")
    (add_net "Net-(R3-Pad1)")
    (add_net "Net-(U1-Pad9)")
    (add_net VCC)
  )

  (module Package_SO:SO-20-1EP_7.52x12.825mm_P1.27mm_EP6.045x12.09mm_Mask3.56x4.47mm (layer B.Cu) (tedit 5DFF42CC) (tstamp 60B032F6)
    (at 123.19 110.49 180)
    (descr "SO, 20 Pin (http://www.ti.com/lit/ds/symlink/opa569.pdf, http://www.ti.com/lit/an/slma004b/slma004b.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SO SO")
    (path /60990192)
    (attr smd)
    (fp_text reference U1 (at 0 7.36) (layer B.SilkS)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text value 74HCT245 (at 0 -7.36) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text user %R (at 0 0) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_line (start 0 -6.5225) (end 3.87 -6.5225) (layer B.SilkS) (width 0.12))
    (fp_line (start 3.87 -6.5225) (end 3.87 -6.275) (layer B.SilkS) (width 0.12))
    (fp_line (start 0 -6.5225) (end -3.87 -6.5225) (layer B.SilkS) (width 0.12))
    (fp_line (start -3.87 -6.5225) (end -3.87 -6.275) (layer B.SilkS) (width 0.12))
    (fp_line (start 0 6.5225) (end 3.87 6.5225) (layer B.SilkS) (width 0.12))
    (fp_line (start 3.87 6.5225) (end 3.87 6.275) (layer B.SilkS) (width 0.12))
    (fp_line (start 0 6.5225) (end -3.87 6.5225) (layer B.SilkS) (width 0.12))
    (fp_line (start -3.87 6.5225) (end -3.87 6.275) (layer B.SilkS) (width 0.12))
    (fp_line (start -3.87 6.275) (end -5.675 6.275) (layer B.SilkS) (width 0.12))
    (fp_line (start -2.76 6.4125) (end 3.76 6.4125) (layer B.Fab) (width 0.1))
    (fp_line (start 3.76 6.4125) (end 3.76 -6.4125) (layer B.Fab) (width 0.1))
    (fp_line (start 3.76 -6.4125) (end -3.76 -6.4125) (layer B.Fab) (width 0.1))
    (fp_line (start -3.76 -6.4125) (end -3.76 5.4125) (layer B.Fab) (width 0.1))
    (fp_line (start -3.76 5.4125) (end -2.76 6.4125) (layer B.Fab) (width 0.1))
    (fp_line (start -5.93 6.66) (end -5.93 -6.66) (layer B.CrtYd) (width 0.05))
    (fp_line (start -5.93 -6.66) (end 5.93 -6.66) (layer B.CrtYd) (width 0.05))
    (fp_line (start 5.93 -6.66) (end 5.93 6.66) (layer B.CrtYd) (width 0.05))
    (fp_line (start 5.93 6.66) (end -5.93 6.66) (layer B.CrtYd) (width 0.05))
    (pad 20 smd roundrect (at 4.675 5.715 180) (size 2 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 27 +5V))
    (pad 19 smd roundrect (at 4.675 4.445 180) (size 2 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 18 smd roundrect (at 4.675 3.175 180) (size 2 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 36 "Net-(J_OUT1-Pad1)"))
    (pad 17 smd roundrect (at 4.675 1.905 180) (size 2 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 37 "Net-(J_OUT1-Pad2)"))
    (pad 16 smd roundrect (at 4.675 0.635 180) (size 2 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 38 "Net-(J_OUT1-Pad3)"))
    (pad 15 smd roundrect (at 4.675 -0.635 180) (size 2 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 39 "Net-(J_OUT1-Pad4)"))
    (pad 14 smd roundrect (at 4.675 -1.905 180) (size 2 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 40 "Net-(J_OUT1-Pad5)"))
    (pad 13 smd roundrect (at 4.675 -3.175 180) (size 2 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 41 "Net-(J_OUT1-Pad6)"))
    (pad 12 smd roundrect (at 4.675 -4.445 180) (size 2 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 42 "Net-(J_OUT1-Pad7)"))
    (pad 11 smd roundrect (at 4.675 -5.715 180) (size 2 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 43 "Net-(J_OUT1-Pad8)"))
    (pad 10 smd roundrect (at -4.675 -5.715 180) (size 2 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 9 smd roundrect (at -4.675 -4.445 180) (size 2 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 57 "Net-(U1-Pad9)"))
    (pad 8 smd roundrect (at -4.675 -3.175 180) (size 2 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 18 /SMI_SD2))
    (pad 7 smd roundrect (at -4.675 -1.905 180) (size 2 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 19 /SMI_SD16))
    (pad 6 smd roundrect (at -4.675 -0.635 180) (size 2 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 22 /SMI_SD14))
    (pad 5 smd roundrect (at -4.675 0.635 180) (size 2 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 21 /SMI_SD15))
    (pad 4 smd roundrect (at -4.675 1.905 180) (size 2 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 24 /SMI_SD9))
    (pad 3 smd roundrect (at -4.675 3.175 180) (size 2 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 25 /SMI_SD7))
    (pad 2 smd roundrect (at -4.675 4.445 180) (size 2 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 26 /SMI_SD6))
    (pad 1 smd roundrect (at -4.675 5.715 180) (size 2 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 55 "Net-(R1-Pad1)"))
    (pad "" smd roundrect (at 0 0 180) (size 2.87 3.6) (layers B.Paste) (roundrect_rratio 0.087108))
    (pad 21 smd roundrect (at 0 0 180) (size 6.045 12.09) (layers B.Cu) (roundrect_rratio 0.041356))
    (pad "" smd roundrect (at 0 0 180) (size 3.56 4.47) (layers B.Mask) (roundrect_rratio 0.070225))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/SO-20-1EP_7.52x12.825mm_P1.27mm_EP6.045x12.09mm_Mask3.56x4.47mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Package_SO:SO-20-1EP_7.52x12.825mm_P1.27mm_EP6.045x12.09mm_Mask3.56x4.47mm (layer B.Cu) (tedit 5DFF42CC) (tstamp 60B003A7)
    (at 123.19 139.7 180)
    (descr "SO, 20 Pin (http://www.ti.com/lit/ds/symlink/opa569.pdf, http://www.ti.com/lit/an/slma004b/slma004b.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SO SO")
    (path /6098F41C)
    (attr smd)
    (fp_text reference U2 (at 0 7.36) (layer B.SilkS)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text value 74HCT245 (at 0 -7.36) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text user %R (at 0 0) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_line (start 0 -6.5225) (end 3.87 -6.5225) (layer B.SilkS) (width 0.12))
    (fp_line (start 3.87 -6.5225) (end 3.87 -6.275) (layer B.SilkS) (width 0.12))
    (fp_line (start 0 -6.5225) (end -3.87 -6.5225) (layer B.SilkS) (width 0.12))
    (fp_line (start -3.87 -6.5225) (end -3.87 -6.275) (layer B.SilkS) (width 0.12))
    (fp_line (start 0 6.5225) (end 3.87 6.5225) (layer B.SilkS) (width 0.12))
    (fp_line (start 3.87 6.5225) (end 3.87 6.275) (layer B.SilkS) (width 0.12))
    (fp_line (start 0 6.5225) (end -3.87 6.5225) (layer B.SilkS) (width 0.12))
    (fp_line (start -3.87 6.5225) (end -3.87 6.275) (layer B.SilkS) (width 0.12))
    (fp_line (start -3.87 6.275) (end -5.675 6.275) (layer B.SilkS) (width 0.12))
    (fp_line (start -2.76 6.4125) (end 3.76 6.4125) (layer B.Fab) (width 0.1))
    (fp_line (start 3.76 6.4125) (end 3.76 -6.4125) (layer B.Fab) (width 0.1))
    (fp_line (start 3.76 -6.4125) (end -3.76 -6.4125) (layer B.Fab) (width 0.1))
    (fp_line (start -3.76 -6.4125) (end -3.76 5.4125) (layer B.Fab) (width 0.1))
    (fp_line (start -3.76 5.4125) (end -2.76 6.4125) (layer B.Fab) (width 0.1))
    (fp_line (start -5.93 6.66) (end -5.93 -6.66) (layer B.CrtYd) (width 0.05))
    (fp_line (start -5.93 -6.66) (end 5.93 -6.66) (layer B.CrtYd) (width 0.05))
    (fp_line (start 5.93 -6.66) (end 5.93 6.66) (layer B.CrtYd) (width 0.05))
    (fp_line (start 5.93 6.66) (end -5.93 6.66) (layer B.CrtYd) (width 0.05))
    (pad 20 smd roundrect (at 4.675 5.715 180) (size 2 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 27 +5V))
    (pad 19 smd roundrect (at 4.675 4.445 180) (size 2 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 18 smd roundrect (at 4.675 3.175 180) (size 2 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 44 "Net-(J_OUT2-Pad1)"))
    (pad 17 smd roundrect (at 4.675 1.905 180) (size 2 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 45 "Net-(J_OUT2-Pad2)"))
    (pad 16 smd roundrect (at 4.675 0.635 180) (size 2 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 46 "Net-(J_OUT2-Pad3)"))
    (pad 15 smd roundrect (at 4.675 -0.635 180) (size 2 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 47 "Net-(J_OUT2-Pad4)"))
    (pad 14 smd roundrect (at 4.675 -1.905 180) (size 2 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 48 "Net-(J_OUT2-Pad5)"))
    (pad 13 smd roundrect (at 4.675 -3.175 180) (size 2 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 49 "Net-(J_OUT2-Pad6)"))
    (pad 12 smd roundrect (at 4.675 -4.445 180) (size 2 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 50 "Net-(J_OUT2-Pad7)"))
    (pad 11 smd roundrect (at 4.675 -5.715 180) (size 2 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 51 "Net-(J_OUT2-Pad8)"))
    (pad 10 smd roundrect (at -4.675 -5.715 180) (size 2 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 9 smd roundrect (at -4.675 -4.445 180) (size 2 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 5 /SMI_SD13))
    (pad 8 smd roundrect (at -4.675 -3.175 180) (size 2 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 8 /SMI_SD8))
    (pad 7 smd roundrect (at -4.675 -1.905 180) (size 2 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 10 /SMI_SD5))
    (pad 6 smd roundrect (at -4.675 -0.635 180) (size 2 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 11 /SMI_SD4))
    (pad 5 smd roundrect (at -4.675 0.635 180) (size 2 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 14 /SMI_SD0))
    (pad 4 smd roundrect (at -4.675 1.905 180) (size 2 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 15 /SMI_SD3))
    (pad 3 smd roundrect (at -4.675 3.175 180) (size 2 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 16 /SMI_SD17))
    (pad 2 smd roundrect (at -4.675 4.445 180) (size 2 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 17 /SMI_SD1))
    (pad 1 smd roundrect (at -4.675 5.715 180) (size 2 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 56 "Net-(R2-Pad2)"))
    (pad "" smd roundrect (at 0 0 180) (size 2.87 3.6) (layers B.Paste) (roundrect_rratio 0.087108))
    (pad 21 smd roundrect (at 0 0 180) (size 6.045 12.09) (layers B.Cu) (roundrect_rratio 0.041356))
    (pad "" smd roundrect (at 0 0 180) (size 3.56 4.47) (layers B.Mask) (roundrect_rratio 0.070225))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/SO-20-1EP_7.52x12.825mm_P1.27mm_EP6.045x12.09mm_Mask3.56x4.47mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Connector_PinSocket_2.54mm:PinSocket_1x05_P2.54mm_Vertical (layer F.Cu) (tedit 5A19A420) (tstamp 60AFE324)
    (at 114.3 119.38)
    (descr "Through hole straight socket strip, 1x05, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x05 2.54mm single row")
    (path /609C0644)
    (fp_text reference SW1 (at 0 -2.77) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value SW_Coded (at 0 12.93) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 5.08 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.27 -1.27) (end 0.635 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start 0.635 -1.27) (end 1.27 -0.635) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 -0.635) (end 1.27 11.43) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 11.43) (end -1.27 11.43) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 11.43) (end -1.27 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.33 1.27) (end 1.33 1.27) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.33 1.27) (end -1.33 11.49) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.33 11.49) (end 1.33 11.49) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.33 1.27) (end 1.33 11.49) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.33 -1.33) (end 1.33 0) (layer F.SilkS) (width 0.12))
    (fp_line (start 0 -1.33) (end 1.33 -1.33) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.8 -1.8) (end 1.75 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.75 -1.8) (end 1.75 11.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.75 11.9) (end -1.8 11.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 11.9) (end -1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 /SEL_MODE3))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 /SEL_MODE2))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 /SEL_MODE1))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 30 /SEL_MODE0))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 29 "Net-(R3-Pad1)"))
    (model ${KISYS3DMOD}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x05_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5AE5139B) (tstamp 60AFE30B)
    (at 114.3 107.95 90)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.167W length 3.6mm diameter 1.6mm")
    (path /609D0F65)
    (fp_text reference R3 (at 3.81 -1.92 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value R (at 3.81 1.92 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 3.81 0 90) (layer F.Fab)
      (effects (font (size 0.72 0.72) (thickness 0.108)))
    )
    (fp_line (start 2.01 -0.8) (end 2.01 0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 2.01 0.8) (end 5.61 0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 5.61 0.8) (end 5.61 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 5.61 -0.8) (end 2.01 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 0 0) (end 2.01 0) (layer F.Fab) (width 0.1))
    (fp_line (start 7.62 0) (end 5.61 0) (layer F.Fab) (width 0.1))
    (fp_line (start 1.89 -0.92) (end 1.89 0.92) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.89 0.92) (end 5.73 0.92) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.73 0.92) (end 5.73 -0.92) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.73 -0.92) (end 1.89 -0.92) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.94 0) (end 1.89 0) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.68 0) (end 5.73 0) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.95 -1.05) (end -0.95 1.05) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.95 1.05) (end 8.57 1.05) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.57 1.05) (end 8.57 -1.05) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.57 -1.05) (end -0.95 -1.05) (layer F.CrtYd) (width 0.05))
    (pad 2 thru_hole oval (at 7.62 0 90) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 20 +3V3))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 29 "Net-(R3-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5AE5139B) (tstamp 60AFE2F4)
    (at 127 101.6 180)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.167W length 3.6mm diameter 1.6mm")
    (path /609B10BD)
    (fp_text reference R1 (at 3.81 -1.92) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value R (at 3.81 1.92) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 3.81 0) (layer F.Fab)
      (effects (font (size 0.72 0.72) (thickness 0.108)))
    )
    (fp_line (start 2.01 -0.8) (end 2.01 0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 2.01 0.8) (end 5.61 0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 5.61 0.8) (end 5.61 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 5.61 -0.8) (end 2.01 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 0 0) (end 2.01 0) (layer F.Fab) (width 0.1))
    (fp_line (start 7.62 0) (end 5.61 0) (layer F.Fab) (width 0.1))
    (fp_line (start 1.89 -0.92) (end 1.89 0.92) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.89 0.92) (end 5.73 0.92) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.73 0.92) (end 5.73 -0.92) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.73 -0.92) (end 1.89 -0.92) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.94 0) (end 1.89 0) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.68 0) (end 5.73 0) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.95 -1.05) (end -0.95 1.05) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.95 1.05) (end 8.57 1.05) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.57 1.05) (end 8.57 -1.05) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.57 -1.05) (end -0.95 -1.05) (layer F.CrtYd) (width 0.05))
    (pad 2 thru_hole oval (at 7.62 0 180) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 27 +5V))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 55 "Net-(R1-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5AE5139B) (tstamp 60AFE2DD)
    (at 119.38 130.81)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.167W length 3.6mm diameter 1.6mm")
    (path /609AF147)
    (fp_text reference R2 (at 3.81 -1.92) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value R (at 3.81 1.92) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 3.81 0) (layer F.Fab)
      (effects (font (size 0.72 0.72) (thickness 0.108)))
    )
    (fp_line (start 2.01 -0.8) (end 2.01 0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 2.01 0.8) (end 5.61 0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 5.61 0.8) (end 5.61 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 5.61 -0.8) (end 2.01 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 0 0) (end 2.01 0) (layer F.Fab) (width 0.1))
    (fp_line (start 7.62 0) (end 5.61 0) (layer F.Fab) (width 0.1))
    (fp_line (start 1.89 -0.92) (end 1.89 0.92) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.89 0.92) (end 5.73 0.92) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.73 0.92) (end 5.73 -0.92) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.73 -0.92) (end 1.89 -0.92) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.94 0) (end 1.89 0) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.68 0) (end 5.73 0) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.95 -1.05) (end -0.95 1.05) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.95 1.05) (end 8.57 1.05) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.57 1.05) (end 8.57 -1.05) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.57 -1.05) (end -0.95 -1.05) (layer F.CrtYd) (width 0.05))
    (pad 2 thru_hole oval (at 7.62 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 56 "Net-(R2-Pad2)"))
    (pad 1 thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 27 +5V))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module LedBarsHat:I2S_MEMS_Microphone (layer F.Cu) (tedit 6099062F) (tstamp 60AFE2C6)
    (at 120.65 127 90)
    (descr "I2S MEMS Microphone")
    (tags "I2S MEMS Microphone")
    (path /609D01E4)
    (fp_text reference MK1 (at 3.81 -2.33 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value MP45DT02 (at 3.81 7.41 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 3.81 2.54 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.635 -1.27) (end 6.985 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start 6.985 -1.27) (end 6.985 6.35) (layer F.Fab) (width 0.1))
    (fp_line (start 6.985 6.35) (end 0.635 6.35) (layer F.Fab) (width 0.1))
    (fp_line (start 0.635 6.35) (end 0.635 -0.27) (layer F.Fab) (width 0.1))
    (fp_line (start 0.635 -0.27) (end 1.635 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.45 -1.55) (end -1.45 6.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 6.6) (end 9.1 6.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start 9.1 6.6) (end 9.1 -1.55) (layer F.CrtYd) (width 0.05))
    (fp_line (start 9.1 -1.55) (end -1.45 -1.55) (layer F.CrtYd) (width 0.05))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 4 thru_hole oval (at 7.62 5.08 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 23 /I2S_CLK))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 /I2S_WS))
    (pad 5 thru_hole oval (at 7.62 2.54 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 /I2S_SD))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 6 thru_hole oval (at 7.62 0 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 20 +3V3))
  )

  (module Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC) (tstamp 60AFE2B2)
    (at 128.27 97.79 90)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (path /60A55661)
    (fp_text reference JP1 (at 0 -2.33 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value Jumper (at 0 4.87 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 1.27) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 -1.27) (end 1.27 3.81) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 3.81) (end -1.27 3.81) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 3.81) (end -1.27 -0.635) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.33 3.87) (end 1.33 3.87) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.33 1.27) (end -1.33 3.87) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.33 1.27) (end 1.33 3.87) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.33 1.27) (end 1.33 1.27) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.33 0) (end -1.33 -1.33) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.33 -1.33) (end 0 -1.33) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.8 -1.8) (end -1.8 4.35) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 4.35) (end 1.8 4.35) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 4.35) (end 1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 27 +5V))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 VCC))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module LedBarsHat:Led_Power_Bus (layer F.Cu) (tedit 609AB8F7) (tstamp 60AFE29C)
    (at 102.87 100.33)
    (descr "Through hole straight pin header, 2x08, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x08 2.54mm double row")
    (path /60A1377F)
    (fp_text reference PWR1 (at 1.27 -2.33) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value Conn_02x08_Row_Letter_Last (at 1.27 20.11) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 1.27 8.89 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 0 -1.27) (end 3.81 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start 3.81 -1.27) (end 3.81 19.05) (layer F.Fab) (width 0.1))
    (fp_line (start 3.81 19.05) (end -1.27 19.05) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 19.05) (end -1.27 0) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 0) (end 0 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.33 19.11) (end 3.87 19.11) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.33 1.27) (end -1.33 19.11) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.87 -1.33) (end 3.87 19.11) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.33 1.27) (end 1.27 1.27) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.27 1.27) (end 1.27 -1.33) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.27 -1.33) (end 3.87 -1.33) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.33 0) (end -1.33 -1.33) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.33 -1.33) (end 0 -1.33) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.8 -1.8) (end -1.8 19.55) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 19.55) (end 4.35 19.55) (layer F.CrtYd) (width 0.05))
    (fp_line (start 4.35 19.55) (end 4.35 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 4.35 -1.8) (end -1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (pad 1a thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 28 +12V))
    (pad 1b thru_hole oval (at 2.54 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2a thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 28 +12V))
    (pad 2b thru_hole oval (at 2.54 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 3a thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 28 +12V))
    (pad 3b thru_hole oval (at 2.54 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 4a thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 28 +12V))
    (pad 4b thru_hole oval (at 2.54 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 5a thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 28 +12V))
    (pad 5b thru_hole oval (at 2.54 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 6a thru_hole oval (at 0 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 28 +12V))
    (pad 6b thru_hole oval (at 2.54 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 7a thru_hole oval (at 0 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 28 +12V))
    (pad 7b thru_hole oval (at 2.54 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 8a thru_hole oval (at 0 17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 28 +12V))
    (pad 8b thru_hole oval (at 2.54 17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
  )

  (module LedBarsHat:Led_Signal_Bus (layer F.Cu) (tedit 609AB921) (tstamp 60AFE276)
    (at 109.22 124.46)
    (descr "Through hole straight socket strip, 1x08, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x08 2.54mm single row")
    (path /60A0C6CA)
    (fp_text reference J_OUT2 (at 0 -2.77) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value Conn_01x08_Female (at 0 20.55) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 8.89 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.8 19.55) (end -1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.75 19.55) (end -1.8 19.55) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.75 -1.8) (end 1.75 19.55) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 -1.8) (end 1.75 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0 -1.33) (end 1.33 -1.33) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.33 -1.33) (end 1.33 0) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.33 1.27) (end 1.33 19.11) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.33 19.11) (end 1.33 19.11) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.33 1.27) (end -1.33 19.11) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.33 1.27) (end 1.33 1.27) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.27 19.05) (end -1.27 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 19.05) (end -1.27 19.05) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 -0.635) (end 1.27 19.05) (layer F.Fab) (width 0.1))
    (fp_line (start 0.635 -1.27) (end 1.27 -0.635) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 -1.27) (end 0.635 -1.27) (layer F.Fab) (width 0.1))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 44 "Net-(J_OUT2-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 45 "Net-(J_OUT2-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 46 "Net-(J_OUT2-Pad3)"))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 47 "Net-(J_OUT2-Pad4)"))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 48 "Net-(J_OUT2-Pad5)"))
    (pad 6 thru_hole oval (at 0 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 49 "Net-(J_OUT2-Pad6)"))
    (pad 7 thru_hole oval (at 0 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 50 "Net-(J_OUT2-Pad7)"))
    (pad 8 thru_hole oval (at 0 17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 51 "Net-(J_OUT2-Pad8)"))
  )

  (module LedBarsHat:Led_Signal_Bus (layer F.Cu) (tedit 609AB921) (tstamp 60AFE25A)
    (at 109.22 100.33)
    (descr "Through hole straight socket strip, 1x08, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x08 2.54mm single row")
    (path /60A0018E)
    (fp_text reference J_OUT1 (at 0 -2.77) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value Conn_01x08_Female (at 0 20.55) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 8.89 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.8 19.55) (end -1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.75 19.55) (end -1.8 19.55) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.75 -1.8) (end 1.75 19.55) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 -1.8) (end 1.75 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0 -1.33) (end 1.33 -1.33) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.33 -1.33) (end 1.33 0) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.33 1.27) (end 1.33 19.11) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.33 19.11) (end 1.33 19.11) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.33 1.27) (end -1.33 19.11) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.33 1.27) (end 1.33 1.27) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.27 19.05) (end -1.27 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 19.05) (end -1.27 19.05) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 -0.635) (end 1.27 19.05) (layer F.Fab) (width 0.1))
    (fp_line (start 0.635 -1.27) (end 1.27 -0.635) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 -1.27) (end 0.635 -1.27) (layer F.Fab) (width 0.1))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 36 "Net-(J_OUT1-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 37 "Net-(J_OUT1-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 38 "Net-(J_OUT1-Pad3)"))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 39 "Net-(J_OUT1-Pad4)"))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 40 "Net-(J_OUT1-Pad5)"))
    (pad 6 thru_hole oval (at 0 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 41 "Net-(J_OUT1-Pad6)"))
    (pad 7 thru_hole oval (at 0 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 42 "Net-(J_OUT1-Pad7)"))
    (pad 8 thru_hole oval (at 0 17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 43 "Net-(J_OUT1-Pad8)"))
  )

  (module LedBarsHat:Led_Power_Bus (layer F.Cu) (tedit 609AB8F7) (tstamp 60AFE23E)
    (at 102.87 124.46)
    (descr "Through hole straight pin header, 2x08, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x08 2.54mm double row")
    (path /60A12108)
    (fp_text reference PWR2 (at 1.27 -2.33) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value Conn_02x08_Row_Letter_Last (at 1.27 20.11) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 1.27 8.89 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 0 -1.27) (end 3.81 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start 3.81 -1.27) (end 3.81 19.05) (layer F.Fab) (width 0.1))
    (fp_line (start 3.81 19.05) (end -1.27 19.05) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 19.05) (end -1.27 0) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 0) (end 0 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.33 19.11) (end 3.87 19.11) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.33 1.27) (end -1.33 19.11) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.87 -1.33) (end 3.87 19.11) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.33 1.27) (end 1.27 1.27) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.27 1.27) (end 1.27 -1.33) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.27 -1.33) (end 3.87 -1.33) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.33 0) (end -1.33 -1.33) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.33 -1.33) (end 0 -1.33) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.8 -1.8) (end -1.8 19.55) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 19.55) (end 4.35 19.55) (layer F.CrtYd) (width 0.05))
    (fp_line (start 4.35 19.55) (end 4.35 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 4.35 -1.8) (end -1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (pad 1a thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 28 +12V))
    (pad 1b thru_hole oval (at 2.54 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2a thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 28 +12V))
    (pad 2b thru_hole oval (at 2.54 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 3a thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 28 +12V))
    (pad 3b thru_hole oval (at 2.54 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 4a thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 28 +12V))
    (pad 4b thru_hole oval (at 2.54 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 5a thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 28 +12V))
    (pad 5b thru_hole oval (at 2.54 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 6a thru_hole oval (at 0 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 28 +12V))
    (pad 6b thru_hole oval (at 2.54 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 7a thru_hole oval (at 0 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 28 +12V))
    (pad 7b thru_hole oval (at 2.54 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 8a thru_hole oval (at 0 17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 28 +12V))
    (pad 8b thru_hole oval (at 2.54 17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
  )

  (module Connector_BarrelJack:BarrelJack_Wuerth_6941xx301002 (layer F.Cu) (tedit 5B191DE1) (tstamp 60AFE218)
    (at 102.87 95.25 180)
    (descr "Wuerth electronics barrel jack connector (5.5mm outher diameter, inner diameter 2.05mm or 2.55mm depending on exact order number), See: http://katalog.we-online.de/em/datasheet/6941xx301002.pdf")
    (tags "connector barrel jack")
    (path /6099631E)
    (fp_text reference IN_12V1 (at 0 -2.5) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value Jack-DC (at 0 15.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 7.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 5 14.1) (end 5 5.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 4.6 5.2) (end 4.6 13.7) (layer F.SilkS) (width 0.12))
    (fp_line (start -4.5 0.1) (end -3.5 -0.9) (layer F.Fab) (width 0.1))
    (fp_line (start 4.5 -0.9) (end -3.5 -0.9) (layer F.Fab) (width 0.1))
    (fp_line (start 4.5 -0.9) (end 4.5 13.6) (layer F.Fab) (width 0.1))
    (fp_line (start 4.5 13.6) (end -4.5 13.6) (layer F.Fab) (width 0.1))
    (fp_line (start -4.5 13.6) (end -4.5 0.1) (layer F.Fab) (width 0.1))
    (fp_line (start 4.6 13.7) (end -4.6 13.7) (layer F.SilkS) (width 0.12))
    (fp_line (start -4.6 13.7) (end -4.6 -1) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.5 -1) (end 4.6 -1) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.6 -1) (end 4.6 0.8) (layer F.SilkS) (width 0.12))
    (fp_line (start -3.2 -1.3) (end -4.9 -1.3) (layer F.SilkS) (width 0.12))
    (fp_line (start -4.9 -1.3) (end -4.9 0.3) (layer F.SilkS) (width 0.12))
    (fp_line (start 5 -1.4) (end -5 -1.4) (layer F.CrtYd) (width 0.05))
    (fp_line (start -5 -1.4) (end -5 14.1) (layer F.CrtYd) (width 0.05))
    (fp_line (start -5 14.1) (end 5 14.1) (layer F.CrtYd) (width 0.05))
    (fp_line (start 5 0.5) (end 5 -1.4) (layer F.CrtYd) (width 0.05))
    (fp_line (start 6.2 0.5) (end 6.2 5.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 6.2 5.5) (end 5 5.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 6.2 0.5) (end 5 0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start -4.6 -1) (end -2.5 -1) (layer F.SilkS) (width 0.12))
    (pad 1 thru_hole rect (at 0 0 180) (size 4.4 1.8) (drill oval 3.4 0.8) (layers *.Cu *.Mask)
      (net 28 +12V))
    (pad 2 thru_hole oval (at 0 5.8 180) (size 4 1.8) (drill oval 3 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 3 thru_hole oval (at 4.8 3 270) (size 4 1.8) (drill oval 3 0.8) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_BarrelJack.3dshapes/BarrelJack_Wuerth_6941xx301002.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC) (tstamp 60AFE1FB)
    (at 111.76 93.98 180)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (path /6099C84A)
    (fp_text reference OUT_12V1 (at 0 -2.33) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value Conn_01x02_Male (at 0 4.87) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 1.27 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 -1.27) (end 1.27 3.81) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 3.81) (end -1.27 3.81) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 3.81) (end -1.27 -0.635) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.33 3.87) (end 1.33 3.87) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.33 1.27) (end -1.33 3.87) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.33 1.27) (end 1.33 3.87) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.33 1.27) (end 1.33 1.27) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.33 0) (end -1.33 -1.33) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.33 -1.33) (end 0 -1.33) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.8 -1.8) (end -1.8 4.35) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 4.35) (end 1.8 4.35) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 4.35) (end 1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 28 +12V))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Connector_PinSocket_2.54mm:PinSocket_2x20_P2.54mm_Vertical (layer B.Cu) (tedit 5A19A433) (tstamp 60AFE1E5)
    (at 137.16 96.52 180)
    (descr "Through hole straight socket strip, 2x20, 2.54mm pitch, double cols (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 2x20 2.54mm double row")
    (path /60988C0F)
    (fp_text reference J1 (at -1.27 2.77) (layer B.SilkS)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text value Raspberry_Pi_2_3 (at -1.27 -51.03) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_line (start -4.34 -50) (end -4.34 1.8) (layer B.CrtYd) (width 0.05))
    (fp_line (start 1.76 -50) (end -4.34 -50) (layer B.CrtYd) (width 0.05))
    (fp_line (start 1.76 1.8) (end 1.76 -50) (layer B.CrtYd) (width 0.05))
    (fp_line (start -4.34 1.8) (end 1.76 1.8) (layer B.CrtYd) (width 0.05))
    (fp_line (start 0 1.33) (end 1.33 1.33) (layer B.SilkS) (width 0.12))
    (fp_line (start 1.33 1.33) (end 1.33 0) (layer B.SilkS) (width 0.12))
    (fp_line (start -1.27 1.33) (end -1.27 -1.27) (layer B.SilkS) (width 0.12))
    (fp_line (start -1.27 -1.27) (end 1.33 -1.27) (layer B.SilkS) (width 0.12))
    (fp_line (start 1.33 -1.27) (end 1.33 -49.59) (layer B.SilkS) (width 0.12))
    (fp_line (start -3.87 -49.59) (end 1.33 -49.59) (layer B.SilkS) (width 0.12))
    (fp_line (start -3.87 1.33) (end -3.87 -49.59) (layer B.SilkS) (width 0.12))
    (fp_line (start -3.87 1.33) (end -1.27 1.33) (layer B.SilkS) (width 0.12))
    (fp_line (start -3.81 -49.53) (end -3.81 1.27) (layer B.Fab) (width 0.1))
    (fp_line (start 1.27 -49.53) (end -3.81 -49.53) (layer B.Fab) (width 0.1))
    (fp_line (start 1.27 0.27) (end 1.27 -49.53) (layer B.Fab) (width 0.1))
    (fp_line (start 0.27 1.27) (end 1.27 0.27) (layer B.Fab) (width 0.1))
    (fp_line (start -3.81 1.27) (end 0.27 1.27) (layer B.Fab) (width 0.1))
    (fp_text user %R (at -1.27 -24.13 270) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 +3V3))
    (pad 2 thru_hole oval (at -2.54 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 27 +5V))
    (pad 3 thru_hole oval (at 0 -2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "Net-(J1-Pad3)"))
    (pad 4 thru_hole oval (at -2.54 -2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 27 +5V))
    (pad 5 thru_hole oval (at 0 -5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "Net-(J1-Pad5)"))
    (pad 6 thru_hole oval (at -2.54 -5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 7 thru_hole oval (at 0 -7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 31 "Net-(J1-Pad7)"))
    (pad 8 thru_hole oval (at -2.54 -7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 26 /SMI_SD6))
    (pad 9 thru_hole oval (at 0 -10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 10 thru_hole oval (at -2.54 -10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 25 /SMI_SD7))
    (pad 11 thru_hole oval (at 0 -12.7 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 24 /SMI_SD9))
    (pad 12 thru_hole oval (at -2.54 -12.7 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 /I2S_CLK))
    (pad 13 thru_hole oval (at 0 -15.24 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 32 "Net-(J1-Pad13)"))
    (pad 14 thru_hole oval (at -2.54 -15.24 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 15 thru_hole oval (at 0 -17.78 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 22 /SMI_SD14))
    (pad 16 thru_hole oval (at -2.54 -17.78 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 /SMI_SD15))
    (pad 17 thru_hole oval (at 0 -20.32 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 +3V3))
    (pad 18 thru_hole oval (at -2.54 -20.32 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 /SMI_SD16))
    (pad 19 thru_hole oval (at 0 -22.86 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 /SMI_SD2))
    (pad 20 thru_hole oval (at -2.54 -22.86 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 21 thru_hole oval (at 0 -25.4 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 /SMI_SD1))
    (pad 22 thru_hole oval (at -2.54 -25.4 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 /SMI_SD17))
    (pad 23 thru_hole oval (at 0 -27.94 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 /SMI_SD3))
    (pad 24 thru_hole oval (at -2.54 -27.94 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 /SMI_SD0))
    (pad 25 thru_hole oval (at 0 -30.48 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 26 thru_hole oval (at -2.54 -30.48 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 33 "Net-(J1-Pad26)"))
    (pad 27 thru_hole oval (at 0 -33.02 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 34 "Net-(J1-Pad27)"))
    (pad 28 thru_hole oval (at -2.54 -33.02 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 35 "Net-(J1-Pad28)"))
    (pad 29 thru_hole oval (at 0 -35.56 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 /SEL_MODE1))
    (pad 30 thru_hole oval (at -2.54 -35.56 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 31 thru_hole oval (at 0 -38.1 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 /SEL_MODE2))
    (pad 32 thru_hole oval (at -2.54 -38.1 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 /SMI_SD4))
    (pad 33 thru_hole oval (at 0 -40.64 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 /SMI_SD5))
    (pad 34 thru_hole oval (at -2.54 -40.64 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 35 thru_hole oval (at 0 -43.18 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 /I2S_WS))
    (pad 36 thru_hole oval (at -2.54 -43.18 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 /SMI_SD8))
    (pad 37 thru_hole oval (at 0 -45.72 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 /SEL_MODE3))
    (pad 38 thru_hole oval (at -2.54 -45.72 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 /I2S_SD))
    (pad 39 thru_hole oval (at 0 -48.26 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 40 thru_hole oval (at -2.54 -48.26 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 /SMI_SD13))
    (model ${KISYS3DMOD}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_2x20_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Connector_PinSocket_2.54mm:PinSocket_1x02_P2.54mm_Vertical (layer F.Cu) (tedit 5A19A420) (tstamp 60AFE1A7)
    (at 118.11 93.98 180)
    (descr "Through hole straight socket strip, 1x02, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x02 2.54mm single row")
    (path /6099CF4C)
    (fp_text reference IN_5V1 (at 0 -2.77) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value Conn_01x02_Female (at 0 5.31) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 1.27 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.27 -1.27) (end 0.635 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start 0.635 -1.27) (end 1.27 -0.635) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 -0.635) (end 1.27 3.81) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 3.81) (end -1.27 3.81) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 3.81) (end -1.27 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.33 1.27) (end 1.33 1.27) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.33 1.27) (end -1.33 3.87) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.33 3.87) (end 1.33 3.87) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.33 1.27) (end 1.33 3.87) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.33 -1.33) (end 1.33 0) (layer F.SilkS) (width 0.12))
    (fp_line (start 0 -1.33) (end 1.33 -1.33) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.8 -1.8) (end 1.75 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.75 -1.8) (end 1.75 4.3) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.75 4.3) (end -1.8 4.3) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 4.3) (end -1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 VCC))
    (model ${KISYS3DMOD}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x02_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Connector_USB:USB_A_CONNFLY_DS1095-WNR0 (layer F.Cu) (tedit 5E39FFBD) (tstamp 60AFE191)
    (at 133.35 92.71 180)
    (descr http://www.connfly.com/userfiles/image/UpLoadFile/File/2013/5/6/DS1095.pdf)
    (tags "USB-A receptacle horizontal through-hole")
    (path /60994FCE)
    (fp_text reference OUT_5V1 (at -1.95 -2.35) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value USB_A (at 3.5 7) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 3.5 5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -3.75 -0.13) (end -3.75 12.99) (layer F.Fab) (width 0.1))
    (fp_line (start 10.75 -1.01) (end 10.75 12.99) (layer F.Fab) (width 0.1))
    (fp_line (start -2.87 -1.01) (end 10.75 -1.01) (layer F.Fab) (width 0.1))
    (fp_line (start -3.75 12.99) (end 10.75 12.99) (layer F.Fab) (width 0.1))
    (fp_line (start -2.87 -1.01) (end -3.75 -0.13) (layer F.Fab) (width 0.1))
    (fp_line (start -5.32 -1.51) (end -5.32 13.49) (layer F.CrtYd) (width 0.05))
    (fp_line (start 12.32 13.49) (end -5.32 13.49) (layer F.CrtYd) (width 0.05))
    (fp_line (start 12.32 -1.51) (end 12.32 13.49) (layer F.CrtYd) (width 0.05))
    (fp_line (start -5.32 -1.51) (end 12.32 -1.51) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.86 4.56) (end -3.86 13.1) (layer F.SilkS) (width 0.12))
    (fp_line (start -3.86 13.1) (end 10.86 13.1) (layer F.SilkS) (width 0.12))
    (fp_line (start 10.86 4.56) (end 10.86 13.1) (layer F.SilkS) (width 0.12))
    (fp_line (start -3.86 -1.12) (end 10.86 -1.12) (layer F.SilkS) (width 0.12))
    (fp_line (start -3.86 -1.12) (end -3.86 0.86) (layer F.SilkS) (width 0.12))
    (fp_line (start 10.86 0.86) (end 10.86 -1.12) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.5 -2) (end 0 -1.5) (layer F.SilkS) (width 0.12))
    (fp_line (start 0 -1.5) (end 0.5 -2) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.5 -2) (end -0.5 -2) (layer F.SilkS) (width 0.12))
    (pad 4 thru_hole circle (at 7 0 180) (size 1.524 1.524) (drill 0.92) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 3 thru_hole circle (at 4.5 0 180) (size 1.524 1.524) (drill 0.92) (layers *.Cu *.Mask)
      (net 52 "Net-(OUT_5V1-Pad3)"))
    (pad 2 thru_hole circle (at 2.5 0 180) (size 1.524 1.524) (drill 0.92) (layers *.Cu *.Mask)
      (net 53 "Net-(OUT_5V1-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.524 1.524) (drill 0.92) (layers *.Cu *.Mask)
      (net 3 VCC))
    (pad 5 thru_hole circle (at -3.07 2.71 180) (size 3.5 3.5) (drill 2.3) (layers *.Cu *.Mask)
      (net 54 "Net-(OUT_5V1-Pad5)"))
    (pad 5 thru_hole circle (at 10.07 2.71 180) (size 3.5 3.5) (drill 2.3) (layers *.Cu *.Mask)
      (net 54 "Net-(OUT_5V1-Pad5)"))
    (model ${KISYS3DMOD}/Connector_USB.3dshapes/USB_A_CONNFLY_DS1095-WNR0.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (segment (start 138.408 121.48) (end 137.494 120.566) (width 0.25) (layer B.Cu) (net 1))
  (segment (start 137.494 120.566) (end 132.226 120.566) (width 0.25) (layer B.Cu) (net 1))
  (segment (start 132.226 120.566) (end 127.865 116.205) (width 0.25) (layer B.Cu) (net 1))
  (segment (start 139.7 119.38) (end 139.7 120.555) (width 0.25) (layer B.Cu) (net 1))
  (segment (start 139.7 120.555) (end 139.333 120.555) (width 0.25) (layer B.Cu) (net 1))
  (segment (start 139.333 120.555) (end 138.408 121.48) (width 0.25) (layer B.Cu) (net 1))
  (segment (start 112.951 91.44) (end 118.11 91.44) (width 0.25) (layer B.Cu) (net 1))
  (segment (start 110.816 98.7557) (end 112.951 96.6214) (width 0.25) (layer B.Cu) (net 1))
  (segment (start 112.951 96.6214) (end 112.951 91.44) (width 0.25) (layer B.Cu) (net 1))
  (segment (start 105.41 100.33) (end 106.585 100.33) (width 0.25) (layer B.Cu) (net 1))
  (segment (start 106.585 100.33) (end 107.761 99.1546) (width 0.25) (layer B.Cu) (net 1))
  (segment (start 107.761 99.1546) (end 110.417 99.1546) (width 0.25) (layer B.Cu) (net 1))
  (segment (start 110.417 99.1546) (end 110.816 98.7557) (width 0.25) (layer B.Cu) (net 1))
  (segment (start 137.16 144.78) (end 128.5 144.78) (width 0.25) (layer B.Cu) (net 1))
  (segment (start 128.5 144.78) (end 127.865 145.415) (width 0.25) (layer B.Cu) (net 1))
  (segment (start 102.87 89.45) (end 108.595 89.45) (width 0.25) (layer B.Cu) (net 1))
  (segment (start 108.595 89.45) (end 110.585 91.44) (width 0.25) (layer B.Cu) (net 1))
  (segment (start 110.585 91.44) (end 111.76 91.44) (width 0.25) (layer B.Cu) (net 1))
  (segment (start 105.41 142.24) (end 105.41 139.7) (width 0.25) (layer F.Cu) (net 1))
  (segment (start 105.41 139.7) (end 105.41 137.16) (width 0.25) (layer F.Cu) (net 1))
  (segment (start 105.41 137.16) (end 105.41 134.62) (width 0.25) (layer F.Cu) (net 1))
  (segment (start 105.41 134.62) (end 105.41 132.08) (width 0.25) (layer F.Cu) (net 1))
  (segment (start 105.41 132.08) (end 105.41 129.54) (width 0.25) (layer F.Cu) (net 1))
  (segment (start 105.41 129.54) (end 105.41 127) (width 0.25) (layer F.Cu) (net 1))
  (segment (start 105.41 127) (end 105.41 124.46) (width 0.25) (layer F.Cu) (net 1))
  (segment (start 105.41 118.11) (end 105.41 115.57) (width 0.25) (layer F.Cu) (net 1))
  (segment (start 105.41 115.57) (end 105.41 113.03) (width 0.25) (layer F.Cu) (net 1))
  (segment (start 105.41 113.03) (end 105.41 110.49) (width 0.25) (layer F.Cu) (net 1))
  (segment (start 105.41 110.49) (end 105.41 107.95) (width 0.25) (layer F.Cu) (net 1))
  (segment (start 105.41 107.95) (end 105.41 105.41) (width 0.25) (layer F.Cu) (net 1))
  (segment (start 105.41 105.41) (end 105.41 102.87) (width 0.25) (layer F.Cu) (net 1))
  (segment (start 105.41 102.87) (end 105.41 100.33) (width 0.25) (layer F.Cu) (net 1))
  (segment (start 112.951 91.44) (end 111.76 91.44) (width 0.25) (layer B.Cu) (net 1))
  (segment (start 110.816 98.7557) (end 118.106 106.045) (width 0.25) (layer B.Cu) (net 1))
  (segment (start 118.106 106.045) (end 118.515 106.045) (width 0.25) (layer B.Cu) (net 1))
  (segment (start 139.7 132.08) (end 139.7 130.905) (width 0.25) (layer F.Cu) (net 1))
  (segment (start 139.7 130.905) (end 139.333 130.905) (width 0.25) (layer F.Cu) (net 1))
  (segment (start 139.333 130.905) (end 138.335 129.907) (width 0.25) (layer F.Cu) (net 1))
  (segment (start 138.335 129.907) (end 138.335 128.983) (width 0.25) (layer F.Cu) (net 1))
  (segment (start 138.335 128.983) (end 137.527 128.175) (width 0.25) (layer F.Cu) (net 1))
  (segment (start 137.527 128.175) (end 137.16 128.175) (width 0.25) (layer F.Cu) (net 1))
  (segment (start 137.16 128.175) (end 137.16 127) (width 0.25) (layer F.Cu) (net 1))
  (segment (start 105.41 124.46) (end 106.585 124.46) (width 0.25) (layer B.Cu) (net 1))
  (segment (start 106.585 124.46) (end 107.761 123.285) (width 0.25) (layer B.Cu) (net 1))
  (segment (start 120.65 127) (end 120.65 128.525) (width 0.25) (layer B.Cu) (net 1))
  (segment (start 117.156 128.525) (end 117.156 134.373) (width 0.25) (layer B.Cu) (net 1))
  (segment (start 117.156 134.373) (end 118.038 135.255) (width 0.25) (layer B.Cu) (net 1))
  (segment (start 118.038 135.255) (end 118.515 135.255) (width 0.25) (layer B.Cu) (net 1))
  (segment (start 126.35 92.71) (end 120.555 92.71) (width 0.25) (layer B.Cu) (net 1))
  (segment (start 120.555 92.71) (end 119.285 91.44) (width 0.25) (layer B.Cu) (net 1))
  (segment (start 119.285 91.44) (end 118.11 91.44) (width 0.25) (layer B.Cu) (net 1))
  (segment (start 117.156 128.525) (end 120.65 128.525) (width 0.25) (layer B.Cu) (net 1))
  (segment (start 120.65 128.525) (end 125.73 128.525) (width 0.25) (layer B.Cu) (net 1))
  (segment (start 125.73 128.525) (end 125.73 127) (width 0.25) (layer B.Cu) (net 1))
  (segment (start 139.7 137.16) (end 139.7 138.335) (width 0.25) (layer F.Cu) (net 1))
  (segment (start 139.7 138.335) (end 140.067 138.335) (width 0.25) (layer F.Cu) (net 1))
  (segment (start 140.067 138.335) (end 140.893 139.161) (width 0.25) (layer F.Cu) (net 1))
  (segment (start 140.893 139.161) (end 140.893 142.721) (width 0.25) (layer F.Cu) (net 1))
  (segment (start 140.893 142.721) (end 140.009 143.605) (width 0.25) (layer F.Cu) (net 1))
  (segment (start 140.009 143.605) (end 139.143 143.605) (width 0.25) (layer F.Cu) (net 1))
  (segment (start 139.143 143.605) (end 138.335 144.413) (width 0.25) (layer F.Cu) (net 1))
  (segment (start 138.335 144.413) (end 138.335 144.78) (width 0.25) (layer F.Cu) (net 1))
  (segment (start 138.335 144.78) (end 137.16 144.78) (width 0.25) (layer F.Cu) (net 1))
  (segment (start 105.41 118.11) (end 105.41 119.285) (width 0.25) (layer B.Cu) (net 1))
  (segment (start 105.41 119.285) (end 107.761 121.636) (width 0.25) (layer B.Cu) (net 1))
  (segment (start 107.761 121.636) (end 107.761 123.285) (width 0.25) (layer B.Cu) (net 1))
  (segment (start 107.761 123.285) (end 110.211 123.285) (width 0.25) (layer B.Cu) (net 1))
  (segment (start 110.211 123.285) (end 112.308 125.381) (width 0.25) (layer B.Cu) (net 1))
  (segment (start 112.308 125.381) (end 112.308 126.685) (width 0.25) (layer B.Cu) (net 1))
  (segment (start 112.308 126.685) (end 113.869 128.246) (width 0.25) (layer B.Cu) (net 1))
  (segment (start 113.869 128.246) (end 116.877 128.246) (width 0.25) (layer B.Cu) (net 1))
  (segment (start 116.877 128.246) (end 117.156 128.525) (width 0.25) (layer B.Cu) (net 1))
  (segment (start 139.7 132.08) (end 139.7 133.255) (width 0.25) (layer B.Cu) (net 1))
  (segment (start 139.7 133.255) (end 140.067 133.255) (width 0.25) (layer B.Cu) (net 1))
  (segment (start 140.067 133.255) (end 140.875 134.063) (width 0.25) (layer B.Cu) (net 1))
  (segment (start 140.875 134.063) (end 140.875 135.177) (width 0.25) (layer B.Cu) (net 1))
  (segment (start 140.875 135.177) (end 140.067 135.985) (width 0.25) (layer B.Cu) (net 1))
  (segment (start 140.067 135.985) (end 139.7 135.985) (width 0.25) (layer B.Cu) (net 1))
  (segment (start 139.7 135.985) (end 139.7 137.16) (width 0.25) (layer B.Cu) (net 1))
  (segment (start 139.7 111.76) (end 139.7 110.585) (width 0.25) (layer F.Cu) (net 1))
  (segment (start 139.7 110.585) (end 140.067 110.585) (width 0.25) (layer F.Cu) (net 1))
  (segment (start 140.067 110.585) (end 140.887 109.765) (width 0.25) (layer F.Cu) (net 1))
  (segment (start 140.887 109.765) (end 140.887 108.741) (width 0.25) (layer F.Cu) (net 1))
  (segment (start 140.887 108.741) (end 140.002 107.855) (width 0.25) (layer F.Cu) (net 1))
  (segment (start 140.002 107.855) (end 139.143 107.855) (width 0.25) (layer F.Cu) (net 1))
  (segment (start 139.143 107.855) (end 138.335 107.047) (width 0.25) (layer F.Cu) (net 1))
  (segment (start 138.335 107.047) (end 138.335 106.68) (width 0.25) (layer F.Cu) (net 1))
  (segment (start 137.16 106.68) (end 138.335 106.68) (width 0.25) (layer F.Cu) (net 1))
  (segment (start 138.335 106.68) (end 138.335 103.773) (width 0.25) (layer F.Cu) (net 1))
  (segment (start 138.335 103.773) (end 139.333 102.775) (width 0.25) (layer F.Cu) (net 1))
  (segment (start 139.333 102.775) (end 139.7 102.775) (width 0.25) (layer F.Cu) (net 1))
  (segment (start 139.7 102.775) (end 139.7 101.6) (width 0.25) (layer F.Cu) (net 1))
  (segment (start 137.16 127) (end 137.16 125.825) (width 0.25) (layer B.Cu) (net 1))
  (segment (start 137.16 125.825) (end 137.527 125.825) (width 0.25) (layer B.Cu) (net 1))
  (segment (start 137.527 125.825) (end 138.335 125.017) (width 0.25) (layer B.Cu) (net 1))
  (segment (start 138.335 125.017) (end 138.335 121.553) (width 0.25) (layer B.Cu) (net 1))
  (segment (start 138.335 121.553) (end 138.408 121.48) (width 0.25) (layer B.Cu) (net 1))
  (segment (start 125.73 127) (end 125.73 125.475) (width 0.25) (layer F.Cu) (net 1))
  (segment (start 125.73 125.475) (end 130.649 120.555) (width 0.25) (layer F.Cu) (net 1))
  (segment (start 130.649 120.555) (end 137.717 120.555) (width 0.25) (layer F.Cu) (net 1))
  (segment (start 137.717 120.555) (end 138.525 119.747) (width 0.25) (layer F.Cu) (net 1))
  (segment (start 138.525 119.747) (end 138.525 119.38) (width 0.25) (layer F.Cu) (net 1))
  (segment (start 139.7 119.38) (end 138.525 119.38) (width 0.25) (layer F.Cu) (net 1))
  (segment (start 138.525 119.38) (end 138.525 113.743) (width 0.25) (layer F.Cu) (net 1))
  (segment (start 138.525 113.743) (end 139.333 112.935) (width 0.25) (layer F.Cu) (net 1))
  (segment (start 139.333 112.935) (end 139.7 112.935) (width 0.25) (layer F.Cu) (net 1))
  (segment (start 139.7 112.935) (end 139.7 111.76) (width 0.25) (layer F.Cu) (net 1))
  (segment (start 133.35 92.71) (end 132.263 92.71) (width 0.25) (layer B.Cu) (net 3))
  (segment (start 132.263 92.71) (end 132.263 92.8459) (width 0.25) (layer B.Cu) (net 3))
  (segment (start 132.263 92.8459) (end 128.494 96.6147) (width 0.25) (layer B.Cu) (net 3))
  (segment (start 128.494 96.6147) (end 128.27 96.6147) (width 0.25) (layer B.Cu) (net 3))
  (segment (start 128.27 97.79) (end 128.27 96.6147) (width 0.25) (layer B.Cu) (net 3))
  (segment (start 118.11 93.98) (end 125.635 93.98) (width 0.25) (layer B.Cu) (net 3))
  (segment (start 125.635 93.98) (end 128.27 96.6147) (width 0.25) (layer B.Cu) (net 3))
  (segment (start 139.7 144.78) (end 138.525 144.78) (width 0.25) (layer B.Cu) (net 5))
  (segment (start 138.525 144.78) (end 138.525 144.413) (width 0.25) (layer B.Cu) (net 5))
  (segment (start 138.525 144.413) (end 137.701 143.589) (width 0.25) (layer B.Cu) (net 5))
  (segment (start 137.701 143.589) (end 128.421 143.589) (width 0.25) (layer B.Cu) (net 5))
  (segment (start 128.421 143.589) (end 127.865 144.145) (width 0.25) (layer B.Cu) (net 5))
  (segment (start 139.7 142.24) (end 139.7 141.065) (width 0.25) (layer F.Cu) (net 6))
  (segment (start 139.7 141.065) (end 139.333 141.065) (width 0.25) (layer F.Cu) (net 6))
  (segment (start 139.333 141.065) (end 138.525 140.257) (width 0.25) (layer F.Cu) (net 6))
  (segment (start 138.525 140.257) (end 138.525 139.364) (width 0.25) (layer F.Cu) (net 6))
  (segment (start 138.525 139.364) (end 137.669 138.508) (width 0.25) (layer F.Cu) (net 6))
  (segment (start 137.669 138.508) (end 133.157 138.508) (width 0.25) (layer F.Cu) (net 6))
  (segment (start 133.157 138.508) (end 124.46 129.81) (width 0.25) (layer F.Cu) (net 6))
  (segment (start 124.46 129.81) (end 124.46 122.175) (width 0.25) (layer F.Cu) (net 6))
  (segment (start 124.46 122.175) (end 123.19 120.905) (width 0.25) (layer F.Cu) (net 6))
  (segment (start 123.19 120.905) (end 123.19 119.38) (width 0.25) (layer F.Cu) (net 6))
  (segment (start 114.3 129.54) (end 115.475 129.54) (width 0.25) (layer F.Cu) (net 7))
  (segment (start 115.475 129.54) (end 128.175 142.24) (width 0.25) (layer F.Cu) (net 7))
  (segment (start 128.175 142.24) (end 137.16 142.24) (width 0.25) (layer F.Cu) (net 7))
  (segment (start 139.7 139.7) (end 138.525 139.7) (width 0.25) (layer B.Cu) (net 8))
  (segment (start 138.525 139.7) (end 138.525 140.067) (width 0.25) (layer B.Cu) (net 8))
  (segment (start 138.525 140.067) (end 137.717 140.875) (width 0.25) (layer B.Cu) (net 8))
  (segment (start 137.717 140.875) (end 133.87 140.875) (width 0.25) (layer B.Cu) (net 8))
  (segment (start 133.87 140.875) (end 131.87 142.875) (width 0.25) (layer B.Cu) (net 8))
  (segment (start 131.87 142.875) (end 127.865 142.875) (width 0.25) (layer B.Cu) (net 8))
  (segment (start 137.16 139.7) (end 133.69 139.7) (width 0.25) (layer F.Cu) (net 9))
  (segment (start 133.69 139.7) (end 123.19 129.2) (width 0.25) (layer F.Cu) (net 9))
  (segment (start 123.19 129.2) (end 123.19 127) (width 0.25) (layer F.Cu) (net 9))
  (segment (start 127.865 141.605) (end 131.54 141.605) (width 0.25) (layer B.Cu) (net 10))
  (segment (start 131.54 141.605) (end 135.985 137.16) (width 0.25) (layer B.Cu) (net 10))
  (segment (start 135.985 137.16) (end 137.16 137.16) (width 0.25) (layer B.Cu) (net 10))
  (segment (start 139.7 134.62) (end 138.525 134.62) (width 0.25) (layer B.Cu) (net 11))
  (segment (start 138.525 134.62) (end 138.525 134.987) (width 0.25) (layer B.Cu) (net 11))
  (segment (start 138.525 134.987) (end 137.717 135.795) (width 0.25) (layer B.Cu) (net 11))
  (segment (start 137.717 135.795) (end 136.037 135.795) (width 0.25) (layer B.Cu) (net 11))
  (segment (start 136.037 135.795) (end 131.498 140.335) (width 0.25) (layer B.Cu) (net 11))
  (segment (start 131.498 140.335) (end 127.865 140.335) (width 0.25) (layer B.Cu) (net 11))
  (segment (start 137.16 134.62) (end 135.985 134.62) (width 0.25) (layer B.Cu) (net 12))
  (segment (start 135.985 134.62) (end 130.905 139.7) (width 0.25) (layer B.Cu) (net 12))
  (segment (start 130.905 139.7) (end 126.809 139.7) (width 0.25) (layer B.Cu) (net 12))
  (segment (start 126.809 139.7) (end 126.539 139.43) (width 0.25) (layer B.Cu) (net 12))
  (segment (start 126.539 139.43) (end 126.539 133.265) (width 0.25) (layer B.Cu) (net 12))
  (segment (start 126.539 133.265) (end 125.935 132.662) (width 0.25) (layer B.Cu) (net 12))
  (segment (start 125.935 132.662) (end 125.935 129.358) (width 0.25) (layer B.Cu) (net 12))
  (segment (start 125.935 129.358) (end 126.869 128.424) (width 0.25) (layer B.Cu) (net 12))
  (segment (start 126.869 128.424) (end 126.869 126.094) (width 0.25) (layer B.Cu) (net 12))
  (segment (start 126.869 126.094) (end 126.25 125.475) (width 0.25) (layer B.Cu) (net 12))
  (segment (start 126.25 125.475) (end 117.001 125.475) (width 0.25) (layer B.Cu) (net 12))
  (segment (start 117.001 125.475) (end 115.475 127) (width 0.25) (layer B.Cu) (net 12))
  (segment (start 115.475 127) (end 114.3 127) (width 0.25) (layer B.Cu) (net 12))
  (segment (start 137.16 132.08) (end 135.985 132.08) (width 0.25) (layer B.Cu) (net 13))
  (segment (start 135.985 132.08) (end 128.365 124.46) (width 0.25) (layer B.Cu) (net 13))
  (segment (start 128.365 124.46) (end 114.3 124.46) (width 0.25) (layer B.Cu) (net 13))
  (segment (start 139.7 124.46) (end 139.7 125.635) (width 0.25) (layer F.Cu) (net 14))
  (segment (start 139.7 125.635) (end 140.067 125.635) (width 0.25) (layer F.Cu) (net 14))
  (segment (start 140.067 125.635) (end 140.889 126.457) (width 0.25) (layer F.Cu) (net 14))
  (segment (start 140.889 126.457) (end 140.889 132.557) (width 0.25) (layer F.Cu) (net 14))
  (segment (start 140.889 132.557) (end 140.096 133.35) (width 0.25) (layer F.Cu) (net 14))
  (segment (start 140.096 133.35) (end 136.002 133.35) (width 0.25) (layer F.Cu) (net 14))
  (segment (start 136.002 133.35) (end 135.35 134.002) (width 0.25) (layer F.Cu) (net 14))
  (segment (start 127.865 139.065) (end 130.287 139.065) (width 0.25) (layer B.Cu) (net 14))
  (segment (start 130.287 139.065) (end 135.35 134.002) (width 0.25) (layer B.Cu) (net 14))
  (via (at 135.35 134.002) (size 0.8) (layers F.Cu B.Cu) (net 14))
  (segment (start 137.16 124.46) (end 137.16 125.635) (width 0.25) (layer F.Cu) (net 15))
  (segment (start 137.16 125.635) (end 136.793 125.635) (width 0.25) (layer F.Cu) (net 15))
  (segment (start 136.793 125.635) (end 131.972 130.456) (width 0.25) (layer F.Cu) (net 15))
  (segment (start 131.972 130.456) (end 131.972 134.6) (width 0.25) (layer F.Cu) (net 15))
  (segment (start 131.972 134.6) (end 128.777 137.795) (width 0.25) (layer B.Cu) (net 15))
  (segment (start 128.777 137.795) (end 127.865 137.795) (width 0.25) (layer B.Cu) (net 15))
  (via (at 131.972 134.6) (size 0.8) (layers F.Cu B.Cu) (net 15))
  (segment (start 139.7 121.92) (end 139.7 123.095) (width 0.25) (layer B.Cu) (net 16))
  (segment (start 139.7 123.095) (end 140.067 123.095) (width 0.25) (layer B.Cu) (net 16))
  (segment (start 140.067 123.095) (end 140.893 123.921) (width 0.25) (layer B.Cu) (net 16))
  (segment (start 140.893 123.921) (end 140.893 127.481) (width 0.25) (layer B.Cu) (net 16))
  (segment (start 140.893 127.481) (end 140.009 128.365) (width 0.25) (layer B.Cu) (net 16))
  (segment (start 140.009 128.365) (end 139.121 128.365) (width 0.25) (layer B.Cu) (net 16))
  (segment (start 139.121 128.365) (end 138.43 129.056) (width 0.25) (layer B.Cu) (net 16))
  (segment (start 138.43 129.056) (end 138.43 132.475) (width 0.25) (layer B.Cu) (net 16))
  (segment (start 138.43 132.475) (end 137.638 133.267) (width 0.25) (layer B.Cu) (net 16))
  (segment (start 137.638 133.267) (end 132.209 133.267) (width 0.25) (layer B.Cu) (net 16))
  (segment (start 132.209 133.267) (end 128.951 136.525) (width 0.25) (layer B.Cu) (net 16))
  (segment (start 128.951 136.525) (end 127.865 136.525) (width 0.25) (layer B.Cu) (net 16))
  (segment (start 137.16 121.92) (end 137.16 123.095) (width 0.25) (layer F.Cu) (net 17))
  (segment (start 137.16 123.095) (end 136.793 123.095) (width 0.25) (layer F.Cu) (net 17))
  (segment (start 136.793 123.095) (end 130.681 129.207) (width 0.25) (layer F.Cu) (net 17))
  (segment (start 130.681 129.207) (end 130.681 132.85) (width 0.25) (layer F.Cu) (net 17))
  (segment (start 130.681 132.85) (end 128.276 135.255) (width 0.25) (layer B.Cu) (net 17))
  (segment (start 128.276 135.255) (end 127.865 135.255) (width 0.25) (layer B.Cu) (net 17))
  (via (at 130.681 132.85) (size 0.8) (layers F.Cu B.Cu) (net 17))
  (segment (start 137.16 119.38) (end 135.985 119.38) (width 0.25) (layer B.Cu) (net 18))
  (segment (start 135.985 119.38) (end 130.27 113.665) (width 0.25) (layer B.Cu) (net 18))
  (segment (start 130.27 113.665) (end 127.865 113.665) (width 0.25) (layer B.Cu) (net 18))
  (segment (start 139.7 116.84) (end 138.525 116.84) (width 0.25) (layer B.Cu) (net 19))
  (segment (start 138.525 116.84) (end 138.525 116.473) (width 0.25) (layer B.Cu) (net 19))
  (segment (start 138.525 116.473) (end 137.717 115.665) (width 0.25) (layer B.Cu) (net 19))
  (segment (start 137.717 115.665) (end 135.261 115.665) (width 0.25) (layer B.Cu) (net 19))
  (segment (start 135.261 115.665) (end 131.991 112.395) (width 0.25) (layer B.Cu) (net 19))
  (segment (start 131.991 112.395) (end 127.865 112.395) (width 0.25) (layer B.Cu) (net 19))
  (segment (start 123.338 104.104) (end 123.338 117.855) (width 0.25) (layer F.Cu) (net 20))
  (segment (start 114.3 100.33) (end 119.564 100.33) (width 0.25) (layer F.Cu) (net 20))
  (segment (start 119.564 100.33) (end 123.338 104.104) (width 0.25) (layer F.Cu) (net 20))
  (segment (start 137.16 96.52) (end 137.16 97.6953) (width 0.25) (layer F.Cu) (net 20))
  (segment (start 137.16 97.6953) (end 135.702 97.6953) (width 0.25) (layer F.Cu) (net 20))
  (segment (start 135.702 97.6953) (end 129.294 104.104) (width 0.25) (layer F.Cu) (net 20))
  (segment (start 129.294 104.104) (end 123.338 104.104) (width 0.25) (layer F.Cu) (net 20))
  (segment (start 120.65 119.38) (end 120.65 117.855) (width 0.25) (layer F.Cu) (net 20))
  (segment (start 120.65 117.855) (end 123.338 117.855) (width 0.25) (layer F.Cu) (net 20))
  (segment (start 137.16 116.84) (end 132.22 116.84) (width 0.25) (layer F.Cu) (net 20))
  (segment (start 132.22 116.84) (end 128.155 120.905) (width 0.25) (layer F.Cu) (net 20))
  (segment (start 128.155 120.905) (end 125.222 120.905) (width 0.25) (layer F.Cu) (net 20))
  (segment (start 125.222 120.905) (end 124.575 120.259) (width 0.25) (layer F.Cu) (net 20))
  (segment (start 124.575 120.259) (end 124.575 118.7) (width 0.25) (layer F.Cu) (net 20))
  (segment (start 124.575 118.7) (end 123.73 117.855) (width 0.25) (layer F.Cu) (net 20))
  (segment (start 123.73 117.855) (end 123.338 117.855) (width 0.25) (layer F.Cu) (net 20))
  (segment (start 139.7 114.3) (end 138.5247 114.3) (width 0.25) (layer B.Cu) (net 21))
  (segment (start 127.865 109.855) (end 131.615 109.855) (width 0.25) (layer B.Cu) (net 21))
  (segment (start 131.615 109.855) (end 134.8847 113.1247) (width 0.25) (layer B.Cu) (net 21))
  (segment (start 134.8847 113.1247) (end 137.7168 113.1247) (width 0.25) (layer B.Cu) (net 21))
  (segment (start 137.7168 113.1247) (end 138.5247 113.9326) (width 0.25) (layer B.Cu) (net 21))
  (segment (start 138.5247 113.9326) (end 138.5247 114.3) (width 0.25) (layer B.Cu) (net 21))
  (segment (start 127.407 109.855) (end 127.865 109.855) (width 0.25) (layer B.Cu) (net 21))
  (segment (start 137.16 114.3) (end 135.3789 114.3) (width 0.25) (layer B.Cu) (net 22))
  (segment (start 135.3789 114.3) (end 132.2039 111.125) (width 0.25) (layer B.Cu) (net 22))
  (segment (start 132.2039 111.125) (end 127.865 111.125) (width 0.25) (layer B.Cu) (net 22))
  (segment (start 139.7 109.22) (end 138.525 109.22) (width 0.25) (layer F.Cu) (net 23))
  (segment (start 138.525 109.22) (end 138.525 109.587) (width 0.25) (layer F.Cu) (net 23))
  (segment (start 138.525 109.587) (end 137.717 110.395) (width 0.25) (layer F.Cu) (net 23))
  (segment (start 137.717 110.395) (end 133.189 110.395) (width 0.25) (layer F.Cu) (net 23))
  (segment (start 133.189 110.395) (end 125.73 117.855) (width 0.25) (layer F.Cu) (net 23))
  (segment (start 125.73 117.855) (end 125.73 119.38) (width 0.25) (layer F.Cu) (net 23))
  (segment (start 137.16 109.22) (end 128.5 109.22) (width 0.25) (layer B.Cu) (net 24))
  (segment (start 128.5 109.22) (end 127.865 108.585) (width 0.25) (layer B.Cu) (net 24))
  (segment (start 139.7 106.68) (end 138.525 106.68) (width 0.25) (layer B.Cu) (net 25))
  (segment (start 138.525 106.68) (end 138.525 107.047) (width 0.25) (layer B.Cu) (net 25))
  (segment (start 138.525 107.047) (end 137.702 107.87) (width 0.25) (layer B.Cu) (net 25))
  (segment (start 137.702 107.87) (end 128.42 107.87) (width 0.25) (layer B.Cu) (net 25))
  (segment (start 128.42 107.87) (end 127.865 107.315) (width 0.25) (layer B.Cu) (net 25))
  (segment (start 139.7 104.14) (end 138.525 104.14) (width 0.25) (layer B.Cu) (net 26))
  (segment (start 138.525 104.14) (end 138.525 104.507) (width 0.25) (layer B.Cu) (net 26))
  (segment (start 138.525 104.507) (end 137.622 105.41) (width 0.25) (layer B.Cu) (net 26))
  (segment (start 137.622 105.41) (end 128.5 105.41) (width 0.25) (layer B.Cu) (net 26))
  (segment (start 128.5 105.41) (end 127.865 106.045) (width 0.25) (layer B.Cu) (net 26))
  (segment (start 139.7 99.06) (end 138.525 99.06) (width 0.25) (layer B.Cu) (net 27))
  (segment (start 138.525 99.06) (end 138.525 98.6927) (width 0.25) (layer B.Cu) (net 27))
  (segment (start 119.38 130.81) (end 118.515 131.675) (width 0.25) (layer B.Cu) (net 27))
  (segment (start 118.515 131.675) (end 118.515 133.985) (width 0.25) (layer B.Cu) (net 27))
  (segment (start 119.38 101.6) (end 119.38 102.625) (width 0.25) (layer B.Cu) (net 27))
  (segment (start 119.38 102.625) (end 118.515 103.49) (width 0.25) (layer B.Cu) (net 27))
  (segment (start 118.515 103.49) (end 118.515 104.775) (width 0.25) (layer B.Cu) (net 27))
  (segment (start 139.7 96.52) (end 139.7 97.6953) (width 0.25) (layer B.Cu) (net 27))
  (segment (start 139.7 97.6953) (end 139.522 97.6953) (width 0.25) (layer B.Cu) (net 27))
  (segment (start 139.522 97.6953) (end 138.525 98.6927) (width 0.25) (layer B.Cu) (net 27))
  (segment (start 119.38 130.81) (end 119.38 101.6) (width 0.25) (layer F.Cu) (net 27))
  (segment (start 119.38 101.6) (end 120.405 101.6) (width 0.25) (layer B.Cu) (net 27))
  (segment (start 120.405 101.6) (end 123.04 98.9653) (width 0.25) (layer B.Cu) (net 27))
  (segment (start 123.04 98.9653) (end 129.268 98.9653) (width 0.25) (layer B.Cu) (net 27))
  (segment (start 129.268 98.9653) (end 129.635 98.5981) (width 0.25) (layer B.Cu) (net 27))
  (segment (start 129.635 98.5981) (end 129.635 97.79) (width 0.25) (layer B.Cu) (net 27))
  (segment (start 129.635 97.79) (end 130.81 97.79) (width 0.25) (layer B.Cu) (net 27))
  (segment (start 130.81 97.79) (end 137.622 97.79) (width 0.25) (layer B.Cu) (net 27))
  (segment (start 137.622 97.79) (end 138.525 98.6927) (width 0.25) (layer B.Cu) (net 27))
  (segment (start 102.87 95.25) (end 102.87 100.33) (width 0.25) (layer F.Cu) (net 28))
  (segment (start 102.87 142.24) (end 102.87 139.7) (width 0.25) (layer F.Cu) (net 28))
  (segment (start 102.87 139.7) (end 102.87 137.16) (width 0.25) (layer F.Cu) (net 28))
  (segment (start 102.87 137.16) (end 102.87 134.62) (width 0.25) (layer F.Cu) (net 28))
  (segment (start 102.87 134.62) (end 102.87 132.08) (width 0.25) (layer F.Cu) (net 28))
  (segment (start 102.87 132.08) (end 102.87 129.54) (width 0.25) (layer F.Cu) (net 28))
  (segment (start 102.87 129.54) (end 102.87 127) (width 0.25) (layer F.Cu) (net 28))
  (segment (start 102.87 118.11) (end 102.87 115.57) (width 0.25) (layer F.Cu) (net 28))
  (segment (start 102.87 115.57) (end 102.87 113.03) (width 0.25) (layer F.Cu) (net 28))
  (segment (start 102.87 113.03) (end 102.87 110.49) (width 0.25) (layer F.Cu) (net 28))
  (segment (start 102.87 110.49) (end 102.87 107.95) (width 0.25) (layer F.Cu) (net 28))
  (segment (start 102.87 107.95) (end 102.87 105.41) (width 0.25) (layer F.Cu) (net 28))
  (segment (start 102.87 105.41) (end 102.87 102.87) (width 0.25) (layer F.Cu) (net 28))
  (segment (start 102.87 102.87) (end 102.87 100.33) (width 0.25) (layer F.Cu) (net 28))
  (segment (start 102.87 95.25) (end 109.315 95.25) (width 0.25) (layer B.Cu) (net 28))
  (segment (start 109.315 95.25) (end 110.585 93.98) (width 0.25) (layer B.Cu) (net 28))
  (segment (start 110.585 93.98) (end 111.76 93.98) (width 0.25) (layer B.Cu) (net 28))
  (segment (start 102.87 118.11) (end 102.87 124.46) (width 0.25) (layer F.Cu) (net 28))
  (segment (start 102.87 124.46) (end 102.87 127) (width 0.25) (layer F.Cu) (net 28))
  (segment (start 114.3 107.95) (end 114.3 119.38) (width 0.25) (layer F.Cu) (net 29))
  (segment (start 109.22 100.33) (end 110.395 100.33) (width 0.25) (layer B.Cu) (net 36))
  (segment (start 110.395 100.33) (end 117.38 107.315) (width 0.25) (layer B.Cu) (net 36))
  (segment (start 117.38 107.315) (end 118.515 107.315) (width 0.25) (layer B.Cu) (net 36))
  (segment (start 109.22 102.87) (end 111.26 102.87) (width 0.25) (layer B.Cu) (net 37))
  (segment (start 111.26 102.87) (end 116.975 108.585) (width 0.25) (layer B.Cu) (net 37))
  (segment (start 116.975 108.585) (end 118.515 108.585) (width 0.25) (layer B.Cu) (net 37))
  (segment (start 109.22 105.41) (end 110.395 105.41) (width 0.25) (layer B.Cu) (net 38))
  (segment (start 110.395 105.41) (end 110.395 105.557) (width 0.25) (layer B.Cu) (net 38))
  (segment (start 110.395 105.557) (end 114.693 109.855) (width 0.25) (layer B.Cu) (net 38))
  (segment (start 114.693 109.855) (end 118.515 109.855) (width 0.25) (layer B.Cu) (net 38))
  (segment (start 109.22 107.95) (end 110.395 107.95) (width 0.25) (layer B.Cu) (net 39))
  (segment (start 110.395 107.95) (end 113.57 111.125) (width 0.25) (layer B.Cu) (net 39))
  (segment (start 113.57 111.125) (end 118.515 111.125) (width 0.25) (layer B.Cu) (net 39))
  (segment (start 109.22 110.49) (end 110.395 110.49) (width 0.25) (layer B.Cu) (net 40))
  (segment (start 110.395 110.49) (end 112.3 112.395) (width 0.25) (layer B.Cu) (net 40))
  (segment (start 112.3 112.395) (end 118.515 112.395) (width 0.25) (layer B.Cu) (net 40))
  (segment (start 109.22 113.03) (end 117.88 113.03) (width 0.25) (layer B.Cu) (net 41))
  (segment (start 117.88 113.03) (end 118.515 113.665) (width 0.25) (layer B.Cu) (net 41))
  (segment (start 109.22 115.57) (end 117.88 115.57) (width 0.25) (layer B.Cu) (net 42))
  (segment (start 117.88 115.57) (end 118.515 114.935) (width 0.25) (layer B.Cu) (net 42))
  (segment (start 109.22 118.11) (end 116.61 118.11) (width 0.25) (layer B.Cu) (net 43))
  (segment (start 116.61 118.11) (end 118.515 116.205) (width 0.25) (layer B.Cu) (net 43))
  (segment (start 109.22 124.46) (end 109.22 125.635) (width 0.25) (layer B.Cu) (net 44))
  (segment (start 109.22 125.635) (end 109.557 125.635) (width 0.25) (layer B.Cu) (net 44))
  (segment (start 109.557 125.635) (end 111.763 127.841) (width 0.25) (layer B.Cu) (net 44))
  (segment (start 111.763 127.841) (end 111.763 130.194) (width 0.25) (layer B.Cu) (net 44))
  (segment (start 111.763 130.194) (end 118.094 136.525) (width 0.25) (layer B.Cu) (net 44))
  (segment (start 118.094 136.525) (end 118.515 136.525) (width 0.25) (layer B.Cu) (net 44))
  (segment (start 109.22 127) (end 109.22 128.175) (width 0.25) (layer B.Cu) (net 45))
  (segment (start 109.22 128.175) (end 109.556 128.175) (width 0.25) (layer B.Cu) (net 45))
  (segment (start 109.556 128.175) (end 111.087 129.707) (width 0.25) (layer B.Cu) (net 45))
  (segment (start 111.087 129.707) (end 111.087 130.841) (width 0.25) (layer B.Cu) (net 45))
  (segment (start 111.087 130.841) (end 118.041 137.795) (width 0.25) (layer B.Cu) (net 45))
  (segment (start 118.041 137.795) (end 118.515 137.795) (width 0.25) (layer B.Cu) (net 45))
  (segment (start 109.22 129.54) (end 109.22 130.715) (width 0.25) (layer B.Cu) (net 46))
  (segment (start 109.22 130.715) (end 109.755 130.715) (width 0.25) (layer B.Cu) (net 46))
  (segment (start 109.755 130.715) (end 118.105 139.065) (width 0.25) (layer B.Cu) (net 46))
  (segment (start 118.105 139.065) (end 118.515 139.065) (width 0.25) (layer B.Cu) (net 46))
  (segment (start 109.22 132.08) (end 110.395 132.08) (width 0.25) (layer B.Cu) (net 47))
  (segment (start 110.395 132.08) (end 110.395 132.735) (width 0.25) (layer B.Cu) (net 47))
  (segment (start 110.395 132.735) (end 117.995 140.335) (width 0.25) (layer B.Cu) (net 47))
  (segment (start 117.995 140.335) (end 118.515 140.335) (width 0.25) (layer B.Cu) (net 47))
  (segment (start 109.22 134.62) (end 110.395 134.62) (width 0.25) (layer B.Cu) (net 48))
  (segment (start 110.395 134.62) (end 117.38 141.605) (width 0.25) (layer B.Cu) (net 48))
  (segment (start 117.38 141.605) (end 118.515 141.605) (width 0.25) (layer B.Cu) (net 48))
  (segment (start 109.22 137.16) (end 110.395 137.16) (width 0.25) (layer B.Cu) (net 49))
  (segment (start 110.395 137.16) (end 116.11 142.875) (width 0.25) (layer B.Cu) (net 49))
  (segment (start 116.11 142.875) (end 118.515 142.875) (width 0.25) (layer B.Cu) (net 49))
  (segment (start 109.22 139.7) (end 110.395 139.7) (width 0.25) (layer B.Cu) (net 50))
  (segment (start 110.395 139.7) (end 114.84 144.145) (width 0.25) (layer B.Cu) (net 50))
  (segment (start 114.84 144.145) (end 118.515 144.145) (width 0.25) (layer B.Cu) (net 50))
  (segment (start 109.22 142.24) (end 110.395 142.24) (width 0.25) (layer B.Cu) (net 51))
  (segment (start 110.395 142.24) (end 113.57 145.415) (width 0.25) (layer B.Cu) (net 51))
  (segment (start 113.57 145.415) (end 118.515 145.415) (width 0.25) (layer B.Cu) (net 51))
  (segment (start 123.28 90) (end 136.42 90) (width 0.25) (layer F.Cu) (net 54))
  (segment (start 127 101.6) (end 127.865 102.465) (width 0.25) (layer B.Cu) (net 55))
  (segment (start 127.865 102.465) (end 127.865 104.775) (width 0.25) (layer B.Cu) (net 55))
  (segment (start 127 130.81) (end 127 131.835) (width 0.25) (layer B.Cu) (net 56))
  (segment (start 127 131.835) (end 127.865 132.7) (width 0.25) (layer B.Cu) (net 56))
  (segment (start 127.865 132.7) (end 127.865 133.985) (width 0.25) (layer B.Cu) (net 56))

)
