
(rules PCB LedBarsHat
  (snap_angle 
    fortyfive_degree
  )
  (autoroute_settings
    (fanout off)
    (autoroute on)
    (postroute on)
    (vias on)
    (via_costs 50)
    (plane_via_costs 5)
    (start_ripup_costs 100)
    (start_pass_no 104)
    (layer_rule F.Cu
      (active on)
      (preferred_direction vertical)
      (preferred_direction_trace_costs 1.0)
      (against_preferred_direction_trace_costs 2.2)
    )
    (layer_rule B.Cu
      (active on)
      (preferred_direction horizontal)
      (preferred_direction_trace_costs 1.0)
      (against_preferred_direction_trace_costs 1.9)
    )
  )
  (rule
    (width 250.0)
    (clear 200.2)
    (clear 125.0 (type smd_to_turn_gap))
    (clear 50.0 (type smd_smd))
  )
  (padstack "Via[0-1]_800:400_um"
    (shape
      (circle F.Cu 800.0 0.0 0.0)
    )
    (shape
      (circle B.Cu 800.0 0.0 0.0)
    )
    (attach off)
  )
  (via 
    "Via[0-1]_800:400_um" "Via[0-1]_800:400_um" default
  )
  (via 
    "Via[0-1]_800:400_um-kicad_default" "Via[0-1]_800:400_um" "kicad_default"
  )
  (via_rule
    default "Via[0-1]_800:400_um"
  )
  (via_rule
    "kicad_default" "Via[0-1]_800:400_um-kicad_default"
  )
  (class default
    (clearance_class default)
    (via_rule default)
    (rule
      (width 250.0)
    )
    (circuit 
      (use_layer F.Cu B.Cu)
    )
  )
  (class "kicad_default"
    GND "Net-(J1-Pad3)" VCC "Net-(J1-Pad5)" "/SMI_SD13" "/I2S_SD" "/SEL_MODE3" "/SMI_SD8"
    "/I2S_WS" "/SMI_SD5" "/SMI_SD4" "/SEL_MODE2" "/SEL_MODE1" "/SMI_SD0" "/SMI_SD3" "/SMI_SD17"
    "/SMI_SD1" "/SMI_SD2" "/SMI_SD16" +3V3 "/SMI_SD15" "/SMI_SD14" "/I2S_CLK" "/SMI_SD9"
    "/SMI_SD7" "/SMI_SD6" +5V +12V "Net-(R3-Pad1)" "/SEL_MODE0" "Net-(J1-Pad7)" "Net-(J1-Pad13)"
    "Net-(J1-Pad26)" "Net-(J1-Pad27)" "Net-(J1-Pad28)" "Net-(J_OUT1-Pad1)" "Net-(J_OUT1-Pad2)" "Net-(J_OUT1-Pad3)" "Net-(J_OUT1-Pad4)" "Net-(J_OUT1-Pad5)"
    "Net-(J_OUT1-Pad6)" "Net-(J_OUT1-Pad7)" "Net-(J_OUT1-Pad8)" "Net-(J_OUT2-Pad1)" "Net-(J_OUT2-Pad2)" "Net-(J_OUT2-Pad3)" "Net-(J_OUT2-Pad4)" "Net-(J_OUT2-Pad5)"
    "Net-(J_OUT2-Pad6)" "Net-(J_OUT2-Pad7)" "Net-(J_OUT2-Pad8)" "Net-(OUT_5V1-Pad3)" "Net-(OUT_5V1-Pad2)" "Net-(OUT_5V1-Pad5)" "Net-(R1-Pad1)" "Net-(R2-Pad2)"
    "Net-(U1-Pad9)"
    (clearance_class "kicad_default")
    (via_rule kicad_default)
    (rule
      (width 250.0)
    )
    (circuit 
      (use_layer F.Cu B.Cu)
    )
  )
)