(kicad_pcb
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "A4")
	(layers
		(0 "F.Cu" signal)
		(31 "B.Cu" signal)
		(32 "B.Adhes" user "B.Adhesive")
		(33 "F.Adhes" user "F.Adhesive")
		(34 "B.Paste" user)
		(35 "F.Paste" user)
		(36 "B.SilkS" user "B.Silkscreen")
		(37 "F.SilkS" user "F.Silkscreen")
		(38 "B.Mask" user)
		(39 "F.Mask" user)
		(40 "Dwgs.User" user "User.Drawings")
		(41 "Cmts.User" user "User.Comments")
		(42 "Eco1.User" user "User.Eco1")
		(43 "Eco2.User" user "User.Eco2")
		(44 "Edge.Cuts" user)
		(45 "Margin" user)
		(46 "B.CrtYd" user "B.Courtyard")
		(47 "F.CrtYd" user "F.Courtyard")
		(48 "B.Fab" user)
		(49 "F.Fab" user)
		(50 "User.1" user)
		(51 "User.2" user)
		(52 "User.3" user)
		(53 "User.4" user)
		(54 "User.5" user)
		(55 "User.6" user)
		(56 "User.7" user)
		(57 "User.8" user)
		(58 "User.9" user)
	)
	(setup
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(pcbplotparams
			(layerselection 0x00010fc_ffffffff)
			(plot_on_all_layers_selection 0x0000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 4)
			(plotframeref no)
			(viasonmask no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plotreference yes)
			(plotvalue yes)
			(plotfptext yes)
			(plotinvisibletext no)
			(sketchpadsonfab no)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 1)
			(scaleselection 1)
			(outputdirectory "")
		)
	)
	(net 0 "")
	(net 1 "VCC")
	(net 2 "/Led_Data")
	(net 3 "unconnected-(D1-DOUT-Pad2)")
	(net 4 "GND")
	(net 5 "/MISO")
	(net 6 "/Rx")
	(net 7 "/RST")
	(net 8 "/MOSI")
	(net 9 "/Sw")
	(net 10 "/Enc_B")
	(net 11 "/Enc_A")
	(net 12 "unconnected-(U1-PA2-Pad11)")
	(net 13 "unconnected-(U1-PB2-Pad5)")
	(net 14 "unconnected-(U1-PA7-Pad6)")
	(net 15 "unconnected-(U1-PA3-Pad10)")
	(footprint "LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm"
		(layer "F.Cu")
		(uuid "36c4710b-1c7d-4a98-965f-c752e294908f")
		(at 128.55 82.15)
		(descr "5.0mm x 5.0mm Addressable RGB LED NeoPixel, https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf")
		(tags "LED RGB NeoPixel PLCC-4 5050")
		(property "Reference" "D1"
			(at 0 -3.5 0)
			(layer "F.SilkS")
			(uuid "32b4ae3f-93ab-4ba0-99c5-b25a9c1bfd1a")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "WS2812B"
			(at 0 4 0)
			(layer "F.Fab")
			(uuid "64e5c123-550f-434e-aba3-3029339d5902")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "9c220770-c11b-4fb6-9e55-3280375c578f")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "76b6a47d-f49f-479c-86a2-dbe0f900c946")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "RGB LED with integrated controller"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "17f60883-47b6-4274-86a6-7322143cfc83")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "LED*WS2812*PLCC*5.0x5.0mm*P3.2mm*")
		(path "/f3d4fef9-eb90-4f27-9d74-c456d739efc7")
		(sheetname "Root")
		(sheetfile "attiny841.kicad_sch")
		(attr smd)
		(fp_line
			(start -3.5 -2.75)
			(end -3.5 2.75)
			(stroke
				(width 0.12)
				(type default)
			)
			(layer "F.SilkS")
			(uuid "799c1ee8-1aad-4295-94b2-54aacc011e82")
		)
		(fp_line
			(start -3.5 -2.75)
			(end 3.5 -2.75)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "79ffea7a-decb-4db0-9006-f26c7c41ff9a")
		)
		(fp_line
			(start -3.5 2.75)
			(end 3.05 2.75)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "3540fa90-5213-4554-bdbf-385b296920c4")
		)
		(fp_line
			(start -2.7 0.9)
			(end -2.7 -0.9)
			(stroke
				(width 0.12)
				(type default)
			)
			(layer "F.SilkS")
			(uuid "81bef6f1-b6d9-4b90-b414-91db4a5dc7ff")
		)
		(fp_line
			(start 2.7 0.9)
			(end 2.7 -0.9)
			(stroke
				(width 0.12)
				(type default)
			)
			(layer "F.SilkS")
			(uuid "278a57e4-112c-42e7-974b-d187e9820475")
		)
		(fp_line
			(start 3.05 2.75)
			(end 3.5 2.3)
			(stroke
				(width 0.12)
				(type default)
			)
			(layer "F.SilkS")
			(uuid "2cde949c-bb03-473d-b986-3f3c7f14cc64")
		)
		(fp_line
			(start 3.5 2.3)
			(end 3.5 -2.75)
			(stroke
				(width 0.12)
				(type default)
			)
			(layer "F.SilkS")
			(uuid "22e20211-f25a-4435-9c67-338c1e2ab8ce")
		)
		(fp_line
			(start -3.45 -2.75)
			(end -3.45 2.75)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "8344f4b6-b7a0-4b76-acc4-eba5e44323b3")
		)
		(fp_line
			(start -3.45 2.75)
			(end 3.45 2.75)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "5248f2b6-6118-4bb2-b48c-312156ef879b")
		)
		(fp_line
			(start 3.45 -2.75)
			(end -3.45 -2.75)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "763997da-17ed-4bcf-bab7-df3620025e88")
		)
		(fp_line
			(start 3.45 2.75)
			(end 3.45 -2.75)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "b9ded607-d9e4-4a1e-ab60-c627f981d9d8")
		)
		(fp_line
			(start -2.5 -2.5)
			(end -2.5 2.5)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "87d2b222-fe3b-4940-a8aa-4185f756f9d2")
		)
		(fp_line
			(start -2.5 2.5)
			(end 2.5 2.5)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "cde74707-9550-4ae2-9fb2-418c73c3f76a")
		)
		(fp_line
			(start 2.5 -2.5)
			(end -2.5 -2.5)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "e46245f0-b999-4303-a6ed-56f82094e9bf")
		)
		(fp_line
			(start 2.5 1.5)
			(end 1.5 2.5)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "056598df-0e0a-4f95-8db1-4de19014ea4c")
		)
		(fp_line
			(start 2.5 2.5)
			(end 2.5 -2.5)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "d4559bad-2f47-4761-b75d-559d161026cc")
		)
		(fp_circle
			(center 0 0)
			(end 0 -2)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill none)
			(layer "F.Fab")
			(uuid "9ead1b54-bf15-456b-b873-2a8eedcd8606")
		)
		(fp_text user "1"
			(at -4 -1.6 0)
			(unlocked yes)
			(layer "F.SilkS")
			(uuid "4f2562c3-b961-430f-8d17-cae77a8d3cd5")
			(effects
				(font
					(size 0.8 0.8)
					(thickness 0.15)
				)
			)
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "2200451e-88ac-403b-9eeb-e92a90613100")
			(effects
				(font
					(size 0.8 0.8)
					(thickness 0.15)
				)
			)
		)
		(pad "1" smd roundrect
			(at -2.45 -1.65)
			(size 1.5 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.1)
			(net 1 "VCC")
			(pinfunction "VDD")
			(pintype "power_in")
			(uuid "0bfb4b40-7703-474c-958d-735fec7f395a")
		)
		(pad "2" smd roundrect
			(at -2.45 1.65)
			(size 1.5 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.1)
			(net 3 "unconnected-(D1-DOUT-Pad2)")
			(pinfunction "DOUT")
			(pintype "output")
			(uuid "82bbcf89-4422-41de-aaca-b33cf224233b")
		)
		(pad "3" smd roundrect
			(at 2.45 1.65)
			(size 1.5 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.1)
			(net 4 "GND")
			(pinfunction "VSS")
			(pintype "power_in")
			(uuid "d8050d1f-9174-4250-bfd1-758efd2a8989")
		)
		(pad "4" smd roundrect
			(at 2.45 -1.65)
			(size 1.5 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.1)
			(net 2 "/Led_Data")
			(pinfunction "DIN")
			(pintype "input")
			(uuid "38889d81-a53e-4bd0-84ca-ab6391fa1043")
		)
		(model "${KICAD8_3DMODEL_DIR}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_2x03_P2.54mm_Vertical"
		(layer "F.Cu")
		(uuid "36ee23a8-ea61-4d3e-9850-a5a3f8b63e8b")
		(at 115.775 101.525 180)
		(descr "Through hole straight pin header, 2x03, 2.54mm pitch, double rows")
		(tags "Through hole pin header THT 2x03 2.54mm double row")
		(property "Reference" "J_ISP1"
			(at 1.27 -2.33 0)
			(layer "F.SilkS")
			(uuid "39cb2fb9-6dd0-4721-85a1-f7d81d74d3fe")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "Conn_02x03_Counter_Clockwise"
			(at 1.27 7.41 0)
			(layer "F.Fab")
			(uuid "94b2ea72-86f9-41af-beaa-877c55516c39")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Connector_PinHeader_2.54mm:PinHeader_2x03_P2.54mm_Vertical"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "beb3cb11-0e9e-43d0-9aac-7a4e8de6d63e")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "aab11c81-89c3-4136-91eb-37a86b5bf859")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Generic connector, double row, 02x03, counter clockwise pin numbering scheme (similar to DIP package numbering), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "ddb694c8-0949-450c-901e-d0f262b94174")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "Connector*:*_2x??_*")
		(path "/2789d9fe-dca3-4fb4-ab0d-ff7687fe8e8f")
		(sheetname "Root")
		(sheetfile "attiny841.kicad_sch")
		(attr through_hole)
		(fp_line
			(start 3.87 -1.33)
			(end 3.87 6.41)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "f98913cd-2b05-457e-8b8c-5cf7a80f8e69")
		)
		(fp_line
			(start 1.27 1.27)
			(end 1.27 -1.33)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "837fd22e-7134-46cd-a379-84267deb5ac4")
		)
		(fp_line
			(start 1.27 -1.33)
			(end 3.87 -1.33)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "8afc59ea-0093-4e3a-ae8e-3eca576416b3")
		)
		(fp_line
			(start -1.33 6.41)
			(end 3.87 6.41)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "8adb6d87-d09f-4549-8b84-82f997e1eba3")
		)
		(fp_line
			(start -1.33 1.27)
			(end 1.27 1.27)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "038681dd-1186-49f7-98e7-eab96c2be20c")
		)
		(fp_line
			(start -1.33 1.27)
			(end -1.33 6.41)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "7cc9f131-8722-4b79-a88f-da463d43a73e")
		)
		(fp_line
			(start -1.33 0)
			(end -1.33 -1.33)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "30cc3c60-402d-49d4-8606-1c0cfd896a7a")
		)
		(fp_line
			(start -1.33 -1.33)
			(end 0 -1.33)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "78c824cf-9337-401f-9464-7cde6807cb4b")
		)
		(fp_line
			(start 4.35 6.85)
			(end 4.35 -1.8)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "b0394a5f-f897-4aa6-8576-15699d9d7dde")
		)
		(fp_line
			(start 4.35 -1.8)
			(end -1.8 -1.8)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "8ef73243-35ef-4987-ab4c-6a095263f70d")
		)
		(fp_line
			(start -1.8 6.85)
			(end 4.35 6.85)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "c449d173-62b8-43f8-a9e5-44c8ef04d7f1")
		)
		(fp_line
			(start -1.8 -1.8)
			(end -1.8 6.85)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "055daddd-d300-4449-a0c5-614adab0dd6d")
		)
		(fp_line
			(start 3.81 6.35)
			(end -1.27 6.35)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "248a1839-f275-431e-bdba-46bbaa6a5e18")
		)
		(fp_line
			(start 3.81 -1.27)
			(end 3.81 6.35)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "e4658b12-80fa-4710-bfd8-7c0ae92167f6")
		)
		(fp_line
			(start 0 -1.27)
			(end 3.81 -1.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "d61fd56a-b412-40bb-937d-4262c489964a")
		)
		(fp_line
			(start -1.27 6.35)
			(end -1.27 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "96c557c7-c22c-4246-8751-3c42dc5dd66d")
		)
		(fp_line
			(start -1.27 0)
			(end 0 -1.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "6cf8b7ce-cdb3-4ae6-ad4d-6b851622c4f2")
		)
		(fp_text user "${REFERENCE}"
			(at 1.27 2.54 90)
			(layer "F.Fab")
			(uuid "98be19c6-41c8-4fe2-8447-dbce4cfc2f81")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" thru_hole rect
			(at 0 0 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "VCC")
			(pinfunction "Pin_1")
			(pintype "passive")
			(uuid "980ed68e-cf93-4034-aede-f3a5fc6b27a0")
		)
		(pad "2" thru_hole oval
			(at 2.54 0 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 8 "/MOSI")
			(pinfunction "Pin_2")
			(pintype "passive")
			(uuid "fd89cd7e-aad2-4a4d-b173-29feaa8c08a4")
		)
		(pad "3" thru_hole oval
			(at 0 2.54 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "GND")
			(pinfunction "Pin_3")
			(pintype "passive")
			(uuid "16d95dc3-d28a-4de2-a8ff-e75cd5b5f464")
		)
		(pad "4" thru_hole oval
			(at 2.54 2.54 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 7 "/RST")
			(pinfunction "Pin_4")
			(pintype "passive")
			(uuid "ee1840c6-cf75-468a-b478-c238f56d5675")
		)
		(pad "5" thru_hole oval
			(at 0 5.08 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "/Rx")
			(pinfunction "Pin_5")
			(pintype "passive")
			(uuid "dac8d111-f883-4675-ae77-ad7463506edb")
		)
		(pad "6" thru_hole oval
			(at 2.54 5.08 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "/MISO")
			(pinfunction "Pin_6")
			(pintype "passive")
			(uuid "432bb8e4-6e91-4f7f-8eb0-7e6276edc862")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x03_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_1x04_P2.54mm_Vertical"
		(layer "F.Cu")
		(uuid "608b8d86-16b6-4c9e-aec2-7a8ee7940cfe")
		(at 136 95.46)
		(descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x04 2.54mm single row")
		(property "Reference" "J_RS1"
			(at 0 -2.33 0)
			(layer "F.SilkS")
			(uuid "09357674-bfb5-4c55-a759-55dbaea3fbff")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "Conn_01x04_Pin"
			(at 0 9.95 0)
			(layer "F.Fab")
			(uuid "695e841c-3256-4568-9699-0d787dc11853")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Connector_PinHeader_2.54mm:PinHeader_1x04_P2.54mm_Vertical"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "db1aa237-87c0-4dfb-8882-eb71d473f6bf")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "8e69d548-de10-48f0-9652-2f07307d2eab")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Generic connector, single row, 01x04, script generated"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "249cd498-7eb8-4c7e-9431-524b6f8747b4")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(path "/3ea1423d-7c5e-40dc-8569-2616a2b44265")
		(sheetname "Root")
		(sheetfile "attiny841.kicad_sch")
		(attr through_hole)
		(fp_line
			(start -1.33 -1.33)
			(end 0 -1.33)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "2e4b1552-ef4b-4c23-b9fc-8a0a99ed4148")
		)
		(fp_line
			(start -1.33 0)
			(end -1.33 -1.33)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "deff80c3-8db4-41c4-9417-6b84c9fffabf")
		)
		(fp_line
			(start -1.33 1.27)
			(end -1.33 8.95)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "0dff7213-5901-426d-af3b-f0649fb8727d")
		)
		(fp_line
			(start -1.33 1.27)
			(end 1.33 1.27)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "faff2fa7-21bf-49fa-a2e7-74bfec429f1b")
		)
		(fp_line
			(start -1.33 8.95)
			(end 1.33 8.95)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "d1923e53-cdd1-4eb4-b3fa-a4daf1c3c582")
		)
		(fp_line
			(start 1.33 1.27)
			(end 1.33 8.95)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "75096717-45d6-4ed0-9601-242ea76f9180")
		)
		(fp_line
			(start -1.8 -1.8)
			(end -1.8 9.4)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "d7c2f983-e929-4d63-9b34-203d82c4e2c0")
		)
		(fp_line
			(start -1.8 9.4)
			(end 1.8 9.4)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "a04b989e-8e86-4cee-aeef-3cf2f0650bfb")
		)
		(fp_line
			(start 1.8 -1.8)
			(end -1.8 -1.8)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "57c85c4f-3647-4404-9f6c-84a9f8f444fd")
		)
		(fp_line
			(start 1.8 9.4)
			(end 1.8 -1.8)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "e6c493d2-799b-40ea-a9c8-3a799be9fa8a")
		)
		(fp_line
			(start -1.27 -0.635)
			(end -0.635 -1.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "d2bf4537-2c4b-49f1-9109-a08dc6a07e7b")
		)
		(fp_line
			(start -1.27 8.89)
			(end -1.27 -0.635)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "11d29308-28df-439a-84be-3e277c5fa8ad")
		)
		(fp_line
			(start -0.635 -1.27)
			(end 1.27 -1.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "b3f19f27-75f7-493d-bf68-a294db157e3b")
		)
		(fp_line
			(start 1.27 -1.27)
			(end 1.27 8.89)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "8b44a4df-49c5-4773-9e4a-584935793120")
		)
		(fp_line
			(start 1.27 8.89)
			(end -1.27 8.89)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "6b6fa9a9-e4a9-444b-b07b-4c8888abea8d")
		)
		(fp_text user "${REFERENCE}"
			(at 0 3.81 90)
			(layer "F.Fab")
			(uuid "1e7077e7-8347-4150-b22c-30db39f17734")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "VCC")
			(pinfunction "Pin_1")
			(pintype "passive")
			(uuid "14a8d792-147c-4218-ba9f-7233a65d31a5")
		)
		(pad "2" thru_hole oval
			(at 0 2.54)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "/Rx")
			(pinfunction "Pin_2")
			(pintype "passive")
			(uuid "2c5fd3fd-2686-4e56-ab7b-0950d2942e49")
		)
		(pad "3" thru_hole oval
			(at 0 5.08)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "/MISO")
			(pinfunction "Pin_3")
			(pintype "passive")
			(uuid "5200fcb1-e546-4f97-bb6b-82b42f532b13")
		)
		(pad "4" thru_hole oval
			(at 0 7.62)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "GND")
			(pinfunction "Pin_4")
			(pintype "passive")
			(uuid "f05905c6-31fd-4e67-86da-2f525b5829db")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x04_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_SO:SOIC-14_3.9x8.7mm_P1.27mm"
		(layer "F.Cu")
		(uuid "750dd647-5cf7-40a8-91ef-8cfd84c5839b")
		(at 109.065 81.8)
		(descr "SOIC, 14 Pin (JEDEC MS-012AB, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_narrow-r/r_14.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOIC SO")
		(property "Reference" "U1"
			(at 0 -5.28 0)
			(layer "F.SilkS")
			(uuid "2f0b7c6d-7e0c-4278-ac4a-6299004f343e")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "ATtiny841-SS"
			(at 0 5.28 0)
			(layer "F.Fab")
			(uuid "8660f0fc-174f-4cfd-b027-263544b70e03")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Package_SO:SOIC-14_3.9x8.7mm_P1.27mm"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "f891e682-0caf-4154-bac4-a61c5e6ed977")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-8495-8-bit-AVR-Microcontrollers-ATtiny441-ATtiny841_Datasheet.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "762b03e8-88db-4485-a20b-b7f158935595")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "16MHz, 8kB Flash, 512B SRAM, 512B EEPROM, ADC, ACI, debugWIRE, SOIC-14"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "4df3f601-d4a2-4ea4-b91a-f3925a8e1b63")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "SOIC*3.9x8.7mm*P1.27mm*")
		(path "/ad8adf82-4671-451d-b028-f6a4047d0fc1")
		(sheetname "Root")
		(sheetfile "attiny841.kicad_sch")
		(attr smd)
		(fp_line
			(start 0 -4.435)
			(end -1.95 -4.435)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "02287dec-28cf-43b6-9bc5-c25bc8f71969")
		)
		(fp_line
			(start 0 -4.435)
			(end 1.95 -4.435)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "4f74a3fc-91f6-41e7-8f0e-54b275f4641a")
		)
		(fp_line
			(start 0 4.435)
			(end -1.95 4.435)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "8fc1579b-5a3a-4230-90cd-648a08db839c")
		)
		(fp_line
			(start 0 4.435)
			(end 1.95 4.435)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "17355b57-4a4f-406b-925e-a2e487915c28")
		)
		(fp_poly
			(pts
				(xy -2.7 -4.37) (xy -2.94 -4.7) (xy -2.46 -4.7) (xy -2.7 -4.37)
			)
			(stroke
				(width 0.12)
				(type solid)
			)
			(fill solid)
			(layer "F.SilkS")
			(uuid "7fb689d1-bd44-4476-a430-42b1a0180fdb")
		)
		(fp_line
			(start -3.7 -4.58)
			(end -3.7 4.58)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "bca319e7-63dc-476b-9db4-11584f7d24f1")
		)
		(fp_line
			(start -3.7 4.58)
			(end 3.7 4.58)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "10925111-1ede-4a24-86b2-2a3c8235cde7")
		)
		(fp_line
			(start 3.7 -4.58)
			(end -3.7 -4.58)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "9fa0571e-80cf-473b-8eb9-a661c6634010")
		)
		(fp_line
			(start 3.7 4.58)
			(end 3.7 -4.58)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "283a6cc2-a939-405b-9168-e22064a8afe4")
		)
		(fp_line
			(start -1.95 -3.35)
			(end -0.975 -4.325)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "1a282975-f0b4-4064-8449-79cbbeee3f13")
		)
		(fp_line
			(start -1.95 4.325)
			(end -1.95 -3.35)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "99f768ee-d67b-4ba9-9d45-0506c068bf49")
		)
		(fp_line
			(start -0.975 -4.325)
			(end 1.95 -4.325)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "923458ab-5958-402f-9a4d-ca3cf2d6825c")
		)
		(fp_line
			(start 1.95 -4.325)
			(end 1.95 4.325)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "de1f718c-1096-422b-b5a0-cd103dedf0a2")
		)
		(fp_line
			(start 1.95 4.325)
			(end -1.95 4.325)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "fc4295b6-f0ca-44df-8011-0c57db23ec7a")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "01bb9e0e-af58-4788-aeb9-1946e1e9445f")
			(effects
				(font
					(size 0.98 0.98)
					(thickness 0.15)
				)
			)
		)
		(pad "1" smd roundrect
			(at -2.475 -3.81)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "VCC")
			(pinfunction "VCC")
			(pintype "power_in")
			(uuid "7e04c77b-53ad-435d-bda9-15587efd56d6")
		)
		(pad "2" smd roundrect
			(at -2.475 -2.54)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 11 "/Enc_A")
			(pinfunction "XTAL1/PB0")
			(pintype "bidirectional")
			(uuid "40069470-d9bd-4666-a585-fb081f5bf887")
		)
		(pad "3" smd roundrect
			(at -2.475 -1.27)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 10 "/Enc_B")
			(pinfunction "XTAL2/PB1")
			(pintype "bidirectional")
			(uuid "f8097c54-70c5-43df-bbe9-ee398c68edb2")
		)
		(pad "4" smd roundrect
			(at -2.475 0)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 7 "/RST")
			(pinfunction "~{RESET}/PB3")
			(pintype "bidirectional")
			(uuid "b07d5bea-ea1e-4222-8813-168dd29369b0")
		)
		(pad "5" smd roundrect
			(at -2.475 1.27)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 13 "unconnected-(U1-PB2-Pad5)")
			(pinfunction "PB2")
			(pintype "bidirectional")
			(uuid "2a5a8016-377f-4d8d-9f90-b1e41bd15fbb")
		)
		(pad "6" smd roundrect
			(at -2.475 2.54)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 14 "unconnected-(U1-PA7-Pad6)")
			(pinfunction "PA7")
			(pintype "bidirectional")
			(uuid "6f853523-5327-426c-b34a-c23e744b1478")
		)
		(pad "7" smd roundrect
			(at -2.475 3.81)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 8 "/MOSI")
			(pinfunction "PA6")
			(pintype "bidirectional")
			(uuid "033c2b35-197c-4f25-ac50-6efb714f05df")
		)
		(pad "8" smd roundrect
			(at 2.475 3.81)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 5 "/MISO")
			(pinfunction "PA5")
			(pintype "bidirectional")
			(uuid "3d4ef4e4-4a29-4ac0-baf9-7fd03d6ab046")
		)
		(pad "9" smd roundrect
			(at 2.475 2.54)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 6 "/Rx")
			(pinfunction "PA4")
			(pintype "bidirectional")
			(uuid "95de6143-58aa-430f-8374-948482f17e16")
		)
		(pad "10" smd roundrect
			(at 2.475 1.27)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 15 "unconnected-(U1-PA3-Pad10)")
			(pinfunction "PA3")
			(pintype "bidirectional")
			(uuid "7d184a53-c71c-4284-98e4-074eba736bc3")
		)
		(pad "11" smd roundrect
			(at 2.475 0)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 12 "unconnected-(U1-PA2-Pad11)")
			(pinfunction "PA2")
			(pintype "bidirectional")
			(uuid "27b66d20-99d7-44de-8f2a-238a0b7a1ae4")
		)
		(pad "12" smd roundrect
			(at 2.475 -1.27)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "/Led_Data")
			(pinfunction "PA1")
			(pintype "bidirectional")
			(uuid "91b572e7-9ed4-46c7-8ad5-08c0c4096939")
		)
		(pad "13" smd roundrect
			(at 2.475 -2.54)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 9 "/Sw")
			(pinfunction "AREF/PA0")
			(pintype "bidirectional")
			(uuid "5348562b-9298-4e4b-9cc2-5e27d695ca21")
		)
		(pad "14" smd roundrect
			(at 2.475 -3.81)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 4 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(uuid "b340ed79-02a7-4f06-982e-d30b52555519")
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_SO.3dshapes/SOIC-14_3.9x8.7mm_P1.27mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Rotary_Encoder:RotaryEncoder_Alps_EC11E-Switch_Vertical_H20mm"
		(layer "F.Cu")
		(uuid "b1b0e734-5ed8-47a8-883e-e90c3120ece6")
		(at 101 63.5)
		(descr "Alps rotary encoder, EC12E... with switch, vertical shaft, http://www.alps.com/prod/info/E/HTML/Encoder/Incremental/EC11/EC11E15204A3.html")
		(tags "rotary encoder")
		(property "Reference" "SW1"
			(at 2.8 -4.7 0)
			(layer "F.SilkS")
			(uuid "f7edb9e5-3a7d-412c-9757-00cceeaae9b4")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "RotaryEncoder_Switch"
			(at 7.5 10.4 0)
			(layer "F.Fab")
			(uuid "abb9fac5-4952-4294-b7ac-d720ae1e084b")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Rotary_Encoder:RotaryEncoder_Alps_EC11E-Switch_Vertical_H20mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "942a194c-30ce-42a9-bec0-064e8a3bb3e8")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "15f6962b-7019-4a8e-bf88-ba678abc2d0f")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Rotary encoder, dual channel, incremental quadrate outputs, with switch"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "7273eb1a-f420-467b-97fd-d7b907314dee")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "RotaryEncoder*Switch*")
		(path "/671ee055-ffab-4ee0-a75a-74d3930c68cf")
		(sheetname "Root")
		(sheetfile "attiny841.kicad_sch")
		(attr through_hole)
		(fp_line
			(start -0.3 -1.6)
			(end 0.3 -1.6)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "c6eed787-9266-401b-84a5-a2be9e18cf1d")
		)
		(fp_line
			(start 0 -1.3)
			(end -0.3 -1.6)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "1761dc0f-7108-4dfd-a5a9-7fe555fcddc5")
		)
		(fp_line
			(start 0.3 -1.6)
			(end 0 -1.3)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "e472e0c0-808c-4b91-a0f4-8830173eadc2")
		)
		(fp_line
			(start 1.4 -3.4)
			(end 1.4 8.4)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "ec77b4b0-d013-43c6-8531-efe8bfaa8751")
		)
		(fp_line
			(start 5.5 -3.4)
			(end 1.4 -3.4)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "59dfb20e-041d-4a3d-902b-a5be5cc48a85")
		)
		(fp_line
			(start 5.5 8.4)
			(end 1.4 8.4)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "6a371f6c-2278-40fa-8806-69a93d759b81")
		)
		(fp_line
			(start 7 2.5)
			(end 8 2.5)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "c41ea30f-6c52-41cc-918d-875d5ae0b2da")
		)
		(fp_line
			(start 7.5 2)
			(end 7.5 3)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "7ff1f3ec-8a1d-4fee-a34e-3cfb1be8267e")
		)
		(fp_line
			(start 9.5 -3.4)
			(end 13.6 -3.4)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "7eda387e-cfa8-4d69-a77a-438476703f63")
		)
		(fp_line
			(start 13.6 -3.4)
			(end 13.6 -1)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "3c5addde-74e9-4ee5-af2c-03aab891307c")
		)
		(fp_line
			(start 13.6 1.2)
			(end 13.6 3.8)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "7173e8d1-8d6a-4afb-9bd0-4c28a7861322")
		)
		(fp_line
			(start 13.6 6)
			(end 13.6 8.4)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "b23487ec-5d67-4ecb-9bc9-f90629c1b5ce")
		)
		(fp_line
			(start 13.6 8.4)
			(end 9.5 8.4)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "273f4ffa-9cc3-4d05-bc40-90caafbd5289")
		)
		(fp_circle
			(center 7.5 2.5)
			(end 10.5 2.5)
			(stroke
				(width 0.12)
				(type solid)
			)
			(fill none)
			(layer "F.SilkS")
			(uuid "46c7eb1a-a4fd-47c3-ac7d-4becf228e4e2")
		)
		(fp_line
			(start -1.5 -4.6)
			(end -1.5 9.6)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "acc94f9a-2685-46ac-b96b-456ee44df175")
		)
		(fp_line
			(start -1.5 -4.6)
			(end 16 -4.6)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "70635bc6-6db1-45fe-8cbf-8e53b0c8431c")
		)
		(fp_line
			(start 16 9.6)
			(end -1.5 9.6)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "7fe33cb9-d6cf-4373-8cfd-89a7784c3752")
		)
		(fp_line
			(start 16 9.6)
			(end 16 -4.6)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "7186201a-54e5-437d-b51a-ee0a9ce31538")
		)
		(fp_line
			(start 1.5 -2.2)
			(end 2.5 -3.3)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "3b55fe51-7595-4680-b04c-2ad65b4ade56")
		)
		(fp_line
			(start 1.5 8.3)
			(end 1.5 -2.2)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "c6e3d8cf-09b8-4592-bd03-f2eb09be6c01")
		)
		(fp_line
			(start 2.5 -3.3)
			(end 13.5 -3.3)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "78cf1205-c7f7-4a3e-bb05-380e485a4e45")
		)
		(fp_line
			(start 4.5 2.5)
			(end 10.5 2.5)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "706d4431-b449-497f-a315-492380b8fb1c")
		)
		(fp_line
			(start 7.5 -0.5)
			(end 7.5 5.5)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "3f6f836d-3f2d-4fdb-9d62-570abc9112a5")
		)
		(fp_line
			(start 13.5 -3.3)
			(end 13.5 8.3)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "72da70fb-fb0c-44f7-bf3d-485156a90fd2")
		)
		(fp_line
			(start 13.5 8.3)
			(end 1.5 8.3)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "54547a42-7f74-4049-b59c-a75ddef71b3c")
		)
		(fp_circle
			(center 7.5 2.5)
			(end 10.5 2.5)
			(stroke
				(width 0.12)
				(type solid)
			)
			(fill none)
			(layer "F.Fab")
			(uuid "f0d5372f-d5a3-4f69-984a-df949a1aee0e")
		)
		(fp_text user "${REFERENCE}"
			(at 11.1 6.3 0)
			(layer "F.Fab")
			(uuid "18ab4912-8a65-4f5c-932b-ece9e0fbf92d")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "A" thru_hole rect
			(at 0 0)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 11 "/Enc_A")
			(pinfunction "A")
			(pintype "passive")
			(uuid "eab605f9-7433-4945-94cd-1bd8bb694121")
		)
		(pad "B" thru_hole circle
			(at 0 5)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "/Enc_B")
			(pinfunction "B")
			(pintype "passive")
			(uuid "e1caa066-4ef8-452c-aee5-c2cdc61369b6")
		)
		(pad "C" thru_hole circle
			(at 0 2.5)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "GND")
			(pinfunction "C")
			(pintype "passive")
			(uuid "dbe3df21-56ee-4cf6-a8e6-c87940d1d478")
		)
		(pad "MP" thru_hole rect
			(at 7.5 -3.1)
			(size 3.2 2)
			(drill oval 2.8 1.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(uuid "a2e1e5a5-c983-42bb-b8f5-44489284db7e")
		)
		(pad "MP" thru_hole rect
			(at 7.5 8.1)
			(size 3.2 2)
			(drill oval 2.8 1.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(uuid "50705917-3e5a-4caa-b5bd-c3eb7c78938e")
		)
		(pad "S1" thru_hole circle
			(at 14.5 5)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "GND")
			(pinfunction "S1")
			(pintype "passive")
			(uuid "c11742ef-a745-46e1-ba14-aa21cf0de816")
		)
		(pad "S2" thru_hole circle
			(at 14.5 0)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 9 "/Sw")
			(pinfunction "S2")
			(pintype "passive")
			(uuid "7315cc4b-8fa3-4681-98d8-0cd505d1a5da")
		)
		(model "${KICAD8_3DMODEL_DIR}/Rotary_Encoder.3dshapes/RotaryEncoder_Alps_EC11E-Switch_Vertical_H20mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(segment
		(start 126.1 80.5)
		(end 129.2861 80.5)
		(width 0.2)
		(layer "F.Cu")
		(net 1)
		(uuid "0e3d5ddf-2dda-4ceb-b291-ab3f6abf045b")
	)
	(segment
		(start 106.9354 77.99)
		(end 110.1104 81.165)
		(width 0.2)
		(layer "F.Cu")
		(net 1)
		(uuid "312f5e4b-f80a-4da2-b875-0d4c218af3f8")
	)
	(segment
		(start 110.1104 81.165)
		(end 112.5641 81.165)
		(width 0.2)
		(layer "F.Cu")
		(net 1)
		(uuid "5616c22b-adad-4112-b41a-583b73ffb25d")
	)
	(segment
		(start 116.9267 85.5276)
		(end 116.9267 99.5096)
		(width 0.2)
		(layer "F.Cu")
		(net 1)
		(uuid "59900821-f528-4ae2-af53-8d0aee7d51b5")
	)
	(segment
		(start 106.59 77.99)
		(end 106.9354 77.99)
		(width 0.2)
		(layer "F.Cu")
		(net 1)
		(uuid "6f13b71b-4669-467f-ae60-7d22d3ce8ed6")
	)
	(segment
		(start 116.063 100.3733)
		(end 115.775 100.3733)
		(width 0.2)
		(layer "F.Cu")
		(net 1)
		(uuid "77e3e2f4-5192-4a84-9f59-fe00f479e9b5")
	)
	(segment
		(start 112.5641 81.165)
		(end 116.9267 85.5276)
		(width 0.2)
		(layer "F.Cu")
		(net 1)
		(uuid "87da85fe-b3b9-4516-9e33-afefa507fd47")
	)
	(segment
		(start 115.775 101.525)
		(end 115.775 100.3733)
		(width 0.2)
		(layer "F.Cu")
		(net 1)
		(uuid "a4824c2d-8945-4ccb-b469-233f828eff41")
	)
	(segment
		(start 121.0724 85.5276)
		(end 116.9267 85.5276)
		(width 0.2)
		(layer "F.Cu")
		(net 1)
		(uuid "ac15b68c-33f4-4d19-9dd9-da4d02055556")
	)
	(segment
		(start 136 87.2139)
		(end 136 95.46)
		(width 0.2)
		(layer "F.Cu")
		(net 1)
		(uuid "bf06313a-052a-4e52-b020-4f1ecc40e591")
	)
	(segment
		(start 129.2861 80.5)
		(end 136 87.2139)
		(width 0.2)
		(layer "F.Cu")
		(net 1)
		(uuid "caa9e1e4-e464-4f74-9f03-db5abd0f9f04")
	)
	(segment
		(start 126.1 80.5)
		(end 121.0724 85.5276)
		(width 0.2)
		(layer "F.Cu")
		(net 1)
		(uuid "dae8ddee-c500-480d-893b-fae384314877")
	)
	(segment
		(start 116.9267 99.5096)
		(end 116.063 100.3733)
		(width 0.2)
		(layer "F.Cu")
		(net 1)
		(uuid "ff1bc56a-093c-4032-ad24-1ec0a75ad65d")
	)
	(segment
		(start 115.0411 80.53)
		(end 115.8431 79.728)
		(width 0.2)
		(layer "F.Cu")
		(net 2)
		(uuid "07082d2a-4b2c-4afc-9078-d34c393fd48f")
	)
	(segment
		(start 111.54 80.53)
		(end 115.0411 80.53)
		(width 0.2)
		(layer "F.Cu")
		(net 2)
		(uuid "29aefca5-28ee-4edb-ba9c-bebfbe1fad7a")
	)
	(segment
		(start 130.228 79.728)
		(end 131 80.5)
		(width 0.2)
		(layer "F.Cu")
		(net 2)
		(uuid "98e3c997-a090-4e07-be1e-ed10ad1ce976")
	)
	(segment
		(start 115.8431 79.728)
		(end 130.228 79.728)
		(width 0.2)
		(layer "F.Cu")
		(net 2)
		(uuid "fee0640c-418b-4b56-83e2-8ef1b689376b")
	)
	(segment
		(start 131 85.0389)
		(end 131 97.1968)
		(width 0.2)
		(layer "F.Cu")
		(net 4)
		(uuid "05b56b76-cfa4-4858-a17b-a59968c89fd5")
	)
	(segment
		(start 136 103.08)
		(end 136 101.9283)
		(width 0.2)
		(layer "F.Cu")
		(net 4)
		(uuid "0b540bb8-bc02-4f6e-9ea4-58e046277988")
	)
	(segment
		(start 131 83.8)
		(end 131 85.0389)
		(width 0.2)
		(layer "F.Cu")
		(net 4)
		(uuid "6952f325-d02c-4a39-afb3-37f872f9e364")
	)
	(segment
		(start 115.5 68.5)
		(end 115.5 74.4067)
		(width 0.2)
		(layer "F.Cu")
		(net 4)
		(uuid "7720c069-bbe8-4429-8317-77401b052f33")
	)
	(segment
		(start 135.7315 101.9283)
		(end 136 101.9283)
		(width 0.2)
		(layer "F.Cu")
		(net 4)
		(uuid "801c6ebc-a913-4c73-9b4a-c1dd5dcdb9da")
	)
	(segment
		(start 115.5 74.4067)
		(end 111.9167 77.99)
		(width 0.2)
		(layer "F.Cu")
		(net 4)
		(uuid "86d0f851-4fb1-49c5-b742-a02dc2ca35af")
	)
	(segment
		(start 111.9167 77.99)
		(end 111.54 77.99)
		(width 0.2)
		(layer "F.Cu")
		(net 4)
		(uuid "b6b6e347-eb0e-4747-8ae4-42ac154e4f38")
	)
	(segment
		(start 113.1068 79.1801)
		(end 111.9167 77.99)
		(width 0.2)
		(layer "F.Cu")
		(net 4)
		(uuid "ba5b1b37-c008-4d6e-ba84-400cfdb699ff")
	)
	(segment
		(start 113.1068 79.3603)
		(end 113.1068 79.1801)
		(width 0.2)
		(layer "F.Cu")
		(net 4)
		(uuid "ec91919f-5cc4-4f27-97cb-815c4acba7e9")
	)
	(segment
		(start 131 97.1968)
		(end 135.7315 101.9283)
		(width 0.2)
		(layer "F.Cu")
		(net 4)
		(uuid "f4b589ea-9102-4fb5-8a07-53b5c8a2d998")
	)
	(via
		(at 113.1068 79.3603)
		(size 0.6)
		(drill 0.3)
		(layers "F.Cu" "B.Cu")
		(net 4)
		(uuid "6ace2112-97b4-4015-9414-d28c74a767bd")
	)
	(via
		(at 131 85.0389)
		(size 0.6)
		(drill 0.3)
		(layers "F.Cu" "B.Cu")
		(net 4)
		(uuid "dc237b49-05a2-4a13-b0a2-bb76e0f6c77b")
	)
	(segment
		(start 101 66)
		(end 103.5 68.5)
		(width 0.2)
		(layer "B.Cu")
		(net 4)
		(uuid "037f28ab-73bd-4b53-99f9-19a81a0f3565")
	)
	(segment
		(start 113.1068 79.3603)
		(end 118.7854 85.0389)
		(width 0.2)
		(layer "B.Cu")
		(net 4)
		(uuid "0919c00f-9965-4d79-bf98-2c5dfe73998c")
	)
	(segment
		(start 136 103.08)
		(end 134.8483 103.08)
		(width 0.2)
		(layer "B.Cu")
		(net 4)
		(uuid "214227ba-1886-4a61-8186-94efc445c54e")
	)
	(segment
		(start 115.775 98.985)
		(end 130.7533 98.985)
		(width 0.2)
		(layer "B.Cu")
		(net 4)
		(uuid "3402c174-abe1-40a3-ac04-cbdf6fbb6d17")
	)
	(segment
		(start 103.5 68.5)
		(end 115.5 68.5)
		(width 0.2)
		(layer "B.Cu")
		(net 4)
		(uuid "6abcd613-6a5c-4dad-baff-3631b0e75256")
	)
	(segment
		(start 118.7854 85.0389)
		(end 131 85.0389)
		(width 0.2)
		(layer "B.Cu")
		(net 4)
		(uuid "b7320f16-44a7-405a-937e-65ccbe87b2e7")
	)
	(segment
		(start 130.7533 98.985)
		(end 134.8483 103.08)
		(width 0.2)
		(layer "B.Cu")
		(net 4)
		(uuid "f2d87d2d-6be4-4084-989f-12db71a20fae")
	)
	(segment
		(start 111.54 85.61)
		(end 113.235 87.305)
		(width 0.2)
		(layer "F.Cu")
		(net 5)
		(uuid "28803b32-f958-4b3c-8d2d-ff1964032ea1")
	)
	(segment
		(start 113.235 87.305)
		(end 113.235 96.445)
		(width 0.2)
		(layer "F.Cu")
		(net 5)
		(uuid "3878f324-b2a9-4f0b-a9e3-2d52292a3daf")
	)
	(segment
		(start 114.3867 96.7135)
		(end 115.3897 97.7165)
		(width 0.2)
		(layer "B.Cu")
		(net 5)
		(uuid "449c9155-de0a-460e-a837-9000eecb367d")
	)
	(segment
		(start 132.0248 97.7165)
		(end 134.8483 100.54)
		(width 0.2)
		(layer "B.Cu")
		(net 5)
		(uuid "4f8476b2-a27c-47a2-ab3b-d9cb9bc4b15c")
	)
	(segment
		(start 113.235 96.445)
		(end 114.3867 96.445)
		(width 0.2)
		(layer "B.Cu")
		(net 5)
		(uuid "5845b3ba-f745-4016-b731-9668c4f664ba")
	)
	(segment
		(start 115.3897 97.7165)
		(end 132.0248 97.7165)
		(width 0.2)
		(layer "B.Cu")
		(net 5)
		(uuid "5b1becb8-322d-4dc7-805d-6a736e5d8d9f")
	)
	(segment
		(start 136 100.54)
		(end 134.8483 100.54)
		(width 0.2)
		(layer "B.Cu")
		(net 5)
		(uuid "b0141f8a-485b-4923-97bf-f725adcaa9f0")
	)
	(segment
		(start 114.3867 96.445)
		(end 114.3867 96.7135)
		(width 0.2)
		(layer "B.Cu")
		(net 5)
		(uuid "ef183c66-2227-4e5f-82df-e9cbb74a0f86")
	)
	(segment
		(start 115.775 88.1763)
		(end 115.775 96.445)
		(width 0.2)
		(layer "F.Cu")
		(net 6)
		(uuid "47fdd1c9-7bd9-4bb7-852c-63a6b4a583d5")
	)
	(segment
		(start 111.54 84.34)
		(end 111.9387 84.34)
		(width 0.2)
		(layer "F.Cu")
		(net 6)
		(uuid "cd31b203-981e-4d2f-8127-d113b6b6fdf5")
	)
	(segment
		(start 111.9387 84.34)
		(end 115.775 88.1763)
		(width 0.2)
		(layer "F.Cu")
		(net 6)
		(uuid "dae95423-9fa0-4803-90a7-b62321254adf")
	)
	(segment
		(start 134.8483 98)
		(end 133.2933 96.445)
		(width 0.2)
		(layer "B.Cu")
		(net 6)
		(uuid "68b1c325-d7f6-42e0-af2f-b6fcd4a5a832")
	)
	(segment
		(start 136 98)
		(end 134.8483 98)
		(width 0.2)
		(layer "B.Cu")
		(net 6)
		(uuid "9b88fbd0-a1ea-4b7d-a207-7f0a82df50f5")
	)
	(segment
		(start 133.2933 96.445)
		(end 115.775 96.445)
		(width 0.2)
		(layer "B.Cu")
		(net 6)
		(uuid "b55de6da-28d5-415a-99fd-16bca9378545")
	)
	(segment
		(start 109.065 83.8236)
		(end 107.0414 81.8)
		(width 0.2)
		(layer "F.Cu")
		(net 7)
		(uuid "4e525a33-3167-44db-9797-afeb5baedffc")
	)
	(segment
		(start 112.9471 97.8333)
		(end 109.065 93.9512)
		(width 0.2)
		(layer "F.Cu")
		(net 7)
		(uuid "53036b64-9f94-43f4-9cc8-9ec25571eef6")
	)
	(segment
		(start 107.0414 81.8)
		(end 106.59 81.8)
		(width 0.2)
		(layer "F.Cu")
		(net 7)
		(uuid "74716072-b2eb-4a13-842c-258868bc4c91")
	)
	(segment
		(start 113.235 97.8333)
		(end 112.9471 97.8333)
		(width 0.2)
		(layer "F.Cu")
		(net 7)
		(uuid "8383cd9e-9c0f-4f2b-886c-43e4a7f7edaa")
	)
	(segment
		(start 113.235 98.985)
		(end 113.235 97.8333)
		(width 0.2)
		(layer "F.Cu")
		(net 7)
		(uuid "f272e25e-1d24-4680-9601-63ce1b695a8f")
	)
	(segment
		(start 109.065 93.9512)
		(end 109.065 83.8236)
		(width 0.2)
		(layer "F.Cu")
		(net 7)
		(uuid "f94975c1-4073-45e6-91eb-7fc07f58c70d")
	)
	(segment
		(start 113.235 100.3733)
		(end 112.9471 100.3733)
		(width 0.2)
		(layer "F.Cu")
		(net 8)
		(uuid "c9b6c538-de6f-4689-8938-060b473f5fbc")
	)
	(segment
		(start 106.59 94.0162)
		(end 106.59 85.61)
		(width 0.2)
		(layer "F.Cu")
		(net 8)
		(uuid "d5cf8fe0-a21c-49ac-8692-355abbb92dd1")
	)
	(segment
		(start 113.235 101.525)
		(end 113.235 100.3733)
		(width 0.2)
		(layer "F.Cu")
		(net 8)
		(uuid "d868aac5-8892-42ee-9a52-09e4d00173c4")
	)
	(segment
		(start 112.9471 100.3733)
		(end 106.59 94.0162)
		(width 0.2)
		(layer "F.Cu")
		(net 8)
		(uuid "dcac7733-c1c2-4e61-9329-a7ef11b13d43")
	)
	(segment
		(start 114.1983 73.4575)
		(end 110.2361 77.4197)
		(width 0.2)
		(layer "F.Cu")
		(net 9)
		(uuid "5c1fcd04-322c-44b7-9879-698b1aaa12f9")
	)
	(segment
		(start 114.1983 64.8017)
		(end 114.1983 73.4575)
		(width 0.2)
		(layer "F.Cu")
		(net 9)
		(uuid "84fe2cc5-d000-4b47-872c-e62bfb2c6fc7")
	)
	(segment
		(start 110.2361 77.4197)
		(end 110.2361 78.3067)
		(width 0.2)
		(layer "F.Cu")
		(net 9)
		(uuid "bd67a605-8bfe-4c3c-b146-b562491f857b")
	)
	(segment
		(start 115.5 63.5)
		(end 114.1983 64.8017)
		(width 0.2)
		(layer "F.Cu")
		(net 9)
		(uuid "cd82b5a8-d1e7-4362-bb00-7c9758b2c133")
	)
	(segment
		(start 110.2361 78.3067)
		(end 111.1894 79.26)
		(width 0.2)
		(layer "F.Cu")
		(net 9)
		(uuid "dc6d8efd-6554-48c8-9c26-ea223370d104")
	)
	(segment
		(start 111.1894 79.26)
		(end 111.54 79.26)
		(width 0.2)
		(layer "F.Cu")
		(net 9)
		(uuid "e878c0c3-ab13-443e-b9bc-f9bfe78f3014")
	)
	(segment
		(start 101 68.5)
		(end 101 75.2923)
		(width 0.2)
		(layer "F.Cu")
		(net 10)
		(uuid "58b6bbb3-5b8b-4953-825b-4e81c7dd86ea")
	)
	(segment
		(start 106.2377 80.53)
		(end 106.59 80.53)
		(width 0.2)
		(layer "F.Cu")
		(net 10)
		(uuid "bd6280c4-7f2b-4776-b0dc-ef5bf8ad4879")
	)
	(segment
		(start 101 75.2923)
		(end 106.2377 80.53)
		(width 0.2)
		(layer "F.Cu")
		(net 10)
		(uuid "c21055c7-367a-4641-b285-f16364cb921f")
	)
	(segment
		(start 105.0212 78.141)
		(end 106.1402 79.26)
		(width 0.2)
		(layer "F.Cu")
		(net 11)
		(uuid "49cca56d-018a-484a-bfaa-180cba99b5e1")
	)
	(segment
		(start 106.1402 79.26)
		(end 106.59 79.26)
		(width 0.2)
		(layer "F.Cu")
		(net 11)
		(uuid "6cc14f78-0a67-4f32-be23-90a9e1421f38")
	)
	(segment
		(start 105.0212 67.5212)
		(end 105.0212 78.141)
		(width 0.2)
		(layer "F.Cu")
		(net 11)
		(uuid "70fd5539-c8fc-453d-a04a-b63ebfb23b84")
	)
	(segment
		(start 101 63.5)
		(end 105.0212 67.5212)
		(width 0.2)
		(layer "F.Cu")
		(net 11)
		(uuid "c8838ab7-5aa8-4eaa-8054-b9ea528e6648")
	)
)
