Processing micro (platform: atmelavr; board: micro; framework: arduino)
-------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------
Verbose mode can be enabled via `-v, --verbose` option
CONFIGURATION: https://docs.platformio.org/page/boards/atmelavr/micro.html
PLATFORM: Atmel AVR > Arduino Micro
HARDWARE: ATMEGA32U4 16MHz 2.50KB RAM (28KB Flash)
Library Dependency Finder -> http://bit.ly/configure-pio-ldf
LDF MODES: FINDER(chain) COMPATIBILITY(soft)
Collected 12 compatible libraries
Scanning dependencies...
Dependency Graph
|-- <MIDI controller> 3.1.0 #e895a51
|   |-- <MIDIUSB> 1.0.3
|   |-- <SoftwareSerial> 1.0
Compiling .pioenvs/micro/src/main.cpp.o
Compiling .pioenvs/micro/lib7af/MIDI controller/MIDI_Outputs/Digital.cpp.o
Compiling .pioenvs/micro/lib7af/MIDI controller/MIDI_Outputs/DigitalCC.cpp.o
Compiling .pioenvs/micro/lib7af/MIDI controller/MIDI_Outputs/DigitalLatch.cpp.o
