(export (version D)
  (design
    (source D:\Windows\Projects\Embedded\LedBars\RpiLedBars\hw\LedBarsHat\LedBarsHat.sch)
    (date "05/10/21 10:56:17")
    (tool "Eeschema (5.1.10)-1")
    (sheet (number 1) (name /) (tstamps /)
      (title_block
        (title LedBarsHat)
        (company)
        (rev)
        (date)
        (source LedBarsHat.sch)
        (comment (number 1) (value ""))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value "")))))
  (components
    (comp (ref U2)
      (value 74HCT245)
      (footprint Package_SO:TSSOP-20_4.4x6.5mm_P0.65mm)
      (libsource (lib 74hct245) (part 74HCT245) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 60990192))
    (comp (ref J4)
      (value Conn_01x02_Male)
      (footprint Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical)
      (datasheet ~)
      (libsource (lib Connector) (part Conn_01x02_Male) (description "Generic connector, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 6099C84A))
    (comp (ref J2)
      (value Conn_01x02_Female)
      (footprint Connector_PinSocket_2.54mm:PinSocket_1x02_P2.54mm_Vertical)
      (datasheet ~)
      (libsource (lib Connector) (part Conn_01x02_Female) (description "Generic connector, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 6099CF4C))
    (comp (ref R2)
      (value R)
      (footprint Resistor_SMD:R_2010_5025Metric_Pad1.40x2.65mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 609B10BD))
    (comp (ref J1)
      (value USB_A)
      (footprint Connector_USB:USB_A_CONNFLY_DS1095-WNR0)
      (datasheet " ~")
      (libsource (lib Connector) (part USB_A) (description "USB Type A connector"))
      (sheetpath (names /) (tstamps /))
      (tstamp 60994FCE))
    (comp (ref R1)
      (value R)
      (footprint Resistor_SMD:R_2010_5025Metric_Pad1.40x2.65mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 609AF147))
    (comp (ref J5)
      (value Jack-DC)
      (footprint Connector_BarrelJack:BarrelJack_Wuerth_6941xx301002)
      (datasheet ~)
      (libsource (lib Connector) (part Jack-DC) (description "DC Barrel Jack"))
      (sheetpath (names /) (tstamps /))
      (tstamp 6099631E))
    (comp (ref MK1)
      (value MP45DT02)
      (footprint Package_DIP:DIP-6_W7.62mm)
      (datasheet http://www.st.com/st-web-ui/static/active/en/resource/technical/document/datasheet/DM00025467.pdf)
      (libsource (lib Sensor_Audio) (part MP45DT02) (description "MEMS Omnidirectional Digital Microphone, HLGA-6"))
      (sheetpath (names /) (tstamps /))
      (tstamp 609D01E4))
    (comp (ref J3)
      (value Raspberry_Pi_2_3)
      (footprint Connector_PinSocket_2.54mm:PinSocket_2x20_P2.54mm_Vertical)
      (datasheet https://www.raspberrypi.org/documentation/hardware/raspberrypi/schematics/rpi_SCH_3bplus_1p0_reduced.pdf)
      (libsource (lib Connector) (part Raspberry_Pi_2_3) (description "expansion header for Raspberry Pi 2 & 3"))
      (sheetpath (names /) (tstamps /))
      (tstamp 60988C0F))
    (comp (ref U1)
      (value 74HCT245)
      (footprint Package_SO:TSSOP-20_4.4x6.5mm_P0.65mm)
      (libsource (lib 74hct245) (part 74HCT245) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 6098F41C)))
  (libparts
    (libpart (lib 74hct245) (part 74HCT245)
      (fields
        (field (name Reference) U)
        (field (name Value) 74HCT245)
        (field (name Footprint) Housings_SOIC:SOIC-20_7.5x12.8mm_Pitch1.27mm))
      (pins
        (pin (num 1) (name A->B) (type input))
        (pin (num 2) (name A0) (type 3state))
        (pin (num 3) (name A1) (type 3state))
        (pin (num 4) (name A2) (type 3state))
        (pin (num 5) (name A3) (type 3state))
        (pin (num 6) (name A4) (type 3state))
        (pin (num 7) (name A5) (type 3state))
        (pin (num 8) (name A6) (type 3state))
        (pin (num 9) (name A7) (type 3state))
        (pin (num 10) (name GND) (type power_in))
        (pin (num 11) (name B7) (type 3state))
        (pin (num 12) (name B6) (type 3state))
        (pin (num 13) (name B5) (type 3state))
        (pin (num 14) (name B4) (type 3state))
        (pin (num 15) (name B3) (type 3state))
        (pin (num 16) (name B2) (type 3state))
        (pin (num 17) (name B1) (type 3state))
        (pin (num 18) (name B0) (type 3state))
        (pin (num 19) (name CE) (type input))
        (pin (num 20) (name VCC) (type power_in))))
    (libpart (lib Connector) (part Barrel_Jack)
      (aliases
        (alias Jack-DC))
      (description "DC Barrel Jack")
      (docs ~)
      (footprints
        (fp BarrelJack*))
      (fields
        (field (name Reference) J)
        (field (name Value) Barrel_Jack))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib Connector) (part Conn_01x02_Female)
      (description "Generic connector, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)")
      (docs ~)
      (footprints
        (fp Connector*:*_1x??_*))
      (fields
        (field (name Reference) J)
        (field (name Value) Conn_01x02_Female))
      (pins
        (pin (num 1) (name Pin_1) (type passive))
        (pin (num 2) (name Pin_2) (type passive))))
    (libpart (lib Connector) (part Conn_01x02_Male)
      (description "Generic connector, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)")
      (docs ~)
      (footprints
        (fp Connector*:*_1x??_*))
      (fields
        (field (name Reference) J)
        (field (name Value) Conn_01x02_Male))
      (pins
        (pin (num 1) (name Pin_1) (type passive))
        (pin (num 2) (name Pin_2) (type passive))))
    (libpart (lib Connector) (part Raspberry_Pi_2_3)
      (description "expansion header for Raspberry Pi 2 & 3")
      (docs https://www.raspberrypi.org/documentation/hardware/raspberrypi/schematics/rpi_SCH_3bplus_1p0_reduced.pdf)
      (footprints
        (fp PinHeader*2x20*P2.54mm*Vertical*)
        (fp PinSocket*2x20*P2.54mm*Vertical*))
      (fields
        (field (name Reference) J)
        (field (name Value) Raspberry_Pi_2_3))
      (pins
        (pin (num 1) (name 3V3) (type power_in))
        (pin (num 2) (name 5V) (type power_in))
        (pin (num 3) (name SDA/GPIO2) (type BiDi))
        (pin (num 4) (name 5V) (type power_in))
        (pin (num 5) (name SCL/GPIO3) (type BiDi))
        (pin (num 6) (name GND) (type power_in))
        (pin (num 7) (name GCLK0/GPIO4) (type BiDi))
        (pin (num 8) (name GPIO14/TXD) (type BiDi))
        (pin (num 9) (name GND) (type power_in))
        (pin (num 10) (name GPIO15/RXD) (type BiDi))
        (pin (num 11) (name GPIO17) (type BiDi))
        (pin (num 12) (name GPIO18/PWM0) (type BiDi))
        (pin (num 13) (name GPIO27) (type BiDi))
        (pin (num 14) (name GND) (type power_in))
        (pin (num 15) (name GPIO22) (type BiDi))
        (pin (num 16) (name GPIO23) (type BiDi))
        (pin (num 17) (name 3V3) (type power_in))
        (pin (num 18) (name GPIO24) (type BiDi))
        (pin (num 19) (name MOSI0/GPIO10) (type BiDi))
        (pin (num 20) (name GND) (type power_in))
        (pin (num 21) (name MISO0/GPIO9) (type BiDi))
        (pin (num 22) (name GPIO25) (type BiDi))
        (pin (num 23) (name SCLK0/GPIO11) (type BiDi))
        (pin (num 24) (name ~CE0~/GPIO8) (type BiDi))
        (pin (num 25) (name GND) (type power_in))
        (pin (num 26) (name ~CE1~/GPIO7) (type BiDi))
        (pin (num 27) (name ID_SD/GPIO0) (type BiDi))
        (pin (num 28) (name ID_SC/GPIO1) (type BiDi))
        (pin (num 29) (name GCLK1/GPIO5) (type BiDi))
        (pin (num 30) (name GND) (type power_in))
        (pin (num 31) (name GCLK2/GPIO6) (type BiDi))
        (pin (num 32) (name PWM0/GPIO12) (type BiDi))
        (pin (num 33) (name PWM1/GPIO13) (type BiDi))
        (pin (num 34) (name GND) (type power_in))
        (pin (num 35) (name GPIO19/MISO1) (type BiDi))
        (pin (num 36) (name GPIO16) (type BiDi))
        (pin (num 37) (name GPIO26) (type BiDi))
        (pin (num 38) (name GPIO20/MOSI1) (type BiDi))
        (pin (num 39) (name GND) (type power_in))
        (pin (num 40) (name GPIO21/SCLK1) (type BiDi))))
    (libpart (lib Connector) (part USB_A)
      (description "USB Type A connector")
      (docs " ~")
      (footprints
        (fp USB*))
      (fields
        (field (name Reference) J)
        (field (name Value) USB_A))
      (pins
        (pin (num 1) (name VBUS) (type power_in))
        (pin (num 2) (name D-) (type BiDi))
        (pin (num 3) (name D+) (type BiDi))
        (pin (num 4) (name GND) (type power_in))
        (pin (num 5) (name Shield) (type passive))))
    (libpart (lib Device) (part R)
      (description Resistor)
      (docs ~)
      (footprints
        (fp R_*))
      (fields
        (field (name Reference) R)
        (field (name Value) R))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib Sensor_Audio) (part MP45DT02)
      (description "MEMS Omnidirectional Digital Microphone, HLGA-6")
      (docs http://www.st.com/st-web-ui/static/active/en/resource/technical/document/datasheet/DM00025467.pdf)
      (footprints
        (fp ST*HLGA*3.76x4.72mm*P1.65mm*))
      (fields
        (field (name Reference) MK)
        (field (name Value) MP45DT02)
        (field (name Footprint) Sensor_Audio:ST_HLGA-6_3.76x4.72mm_P1.65mm))
      (pins
        (pin (num 1) (name GND) (type power_in))
        (pin (num 2) (name LR) (type input))
        (pin (num 3) (name GND) (type passive))
        (pin (num 4) (name CLK) (type input))
        (pin (num 5) (name DOUT) (type output))
        (pin (num 6) (name VDD) (type power_in)))))
  (libraries
    (library (logical 74hct245)
      (uri D:/Windows/Paquito/Downloads/myelin-kicad-libraries-master/74hct245.lib))
    (library (logical Connector)
      (uri "C:\\Program Files\\KiCad\\share\\kicad\\library/Connector.lib"))
    (library (logical Device)
      (uri "C:\\Program Files\\KiCad\\share\\kicad\\library/Device.lib"))
    (library (logical Sensor_Audio)
      (uri "C:\\Program Files\\KiCad\\share\\kicad\\library/Sensor_Audio.lib")))
  (nets
    (net (code 1) (name VCC)
      (node (ref R2) (pin 2))
      (node (ref J2) (pin 1))
      (node (ref U2) (pin 20))
      (node (ref J1) (pin 1))
      (node (ref U1) (pin 20))
      (node (ref J3) (pin 4))
      (node (ref J3) (pin 2))
      (node (ref R1) (pin 1)))
    (net (code 2) (name GND)
      (node (ref J1) (pin 4))
      (node (ref U2) (pin 10))
      (node (ref J3) (pin 9))
      (node (ref J3) (pin 6))
      (node (ref J3) (pin 39))
      (node (ref J3) (pin 34))
      (node (ref J3) (pin 20))
      (node (ref J3) (pin 30))
      (node (ref J3) (pin 25))
      (node (ref U1) (pin 19))
      (node (ref J5) (pin 2))
      (node (ref J2) (pin 2))
      (node (ref J4) (pin 2))
      (node (ref U2) (pin 19))
      (node (ref J3) (pin 14))
      (node (ref U1) (pin 10))
      (node (ref MK1) (pin 3))
      (node (ref MK1) (pin 1)))
    (net (code 3) (name /I2S_WS)
      (node (ref J3) (pin 35))
      (node (ref MK1) (pin 2)))
    (net (code 4) (name /I2S_SD)
      (node (ref MK1) (pin 5))
      (node (ref J3) (pin 38)))
    (net (code 5) (name /SMI_SD15)
      (node (ref J3) (pin 16))
      (node (ref U2) (pin 4)))
    (net (code 6) (name /SMI_SD14)
      (node (ref U1) (pin 8))
      (node (ref J3) (pin 15)))
    (net (code 7) (name "Net-(J3-Pad13)")
      (node (ref J3) (pin 13)))
    (net (code 8) (name /I2S_CLK)
      (node (ref MK1) (pin 4))
      (node (ref J3) (pin 12)))
    (net (code 9) (name /SMI_SD9)
      (node (ref U1) (pin 9))
      (node (ref J3) (pin 11)))
    (net (code 10) (name /SMI_SD7)
      (node (ref J3) (pin 10))
      (node (ref U2) (pin 3)))
    (net (code 11) (name +3V3)
      (node (ref MK1) (pin 6))
      (node (ref J3) (pin 17))
      (node (ref J3) (pin 1)))
    (net (code 12) (name "Net-(J3-Pad27)")
      (node (ref J3) (pin 27)))
    (net (code 13) (name "Net-(J3-Pad37)")
      (node (ref J3) (pin 37)))
    (net (code 14) (name "Net-(J3-Pad28)")
      (node (ref J3) (pin 28)))
    (net (code 15) (name "Net-(J3-Pad26)")
      (node (ref J3) (pin 26)))
    (net (code 16) (name /SMI_SD16)
      (node (ref U2) (pin 5))
      (node (ref J3) (pin 18)))
    (net (code 17) (name "Net-(J3-Pad3)")
      (node (ref J3) (pin 3)))
    (net (code 18) (name "Net-(J3-Pad5)")
      (node (ref J3) (pin 5)))
    (net (code 19) (name "Net-(J3-Pad7)")
      (node (ref J3) (pin 7)))
    (net (code 20) (name "Net-(J3-Pad29)")
      (node (ref J3) (pin 29)))
    (net (code 21) (name "Net-(J3-Pad31)")
      (node (ref J3) (pin 31)))
    (net (code 22) (name +12V)
      (node (ref J4) (pin 1))
      (node (ref J5) (pin 1)))
    (net (code 23) (name "Net-(R1-Pad2)")
      (node (ref R1) (pin 2))
      (node (ref U1) (pin 1)))
    (net (code 24) (name "Net-(U1-Pad15)")
      (node (ref U1) (pin 15)))
    (net (code 25) (name "Net-(U1-Pad18)")
      (node (ref U1) (pin 18)))
    (net (code 26) (name "Net-(U1-Pad17)")
      (node (ref U1) (pin 17)))
    (net (code 27) (name "Net-(U1-Pad16)")
      (node (ref U1) (pin 16)))
    (net (code 28) (name "Net-(U1-Pad14)")
      (node (ref U1) (pin 14)))
    (net (code 29) (name "Net-(U1-Pad13)")
      (node (ref U1) (pin 13)))
    (net (code 30) (name "Net-(U1-Pad12)")
      (node (ref U1) (pin 12)))
    (net (code 31) (name "Net-(U1-Pad11)")
      (node (ref U1) (pin 11)))
    (net (code 32) (name /SMI_SD4)
      (node (ref J3) (pin 32))
      (node (ref U2) (pin 8)))
    (net (code 33) (name /SMI_SD5)
      (node (ref J3) (pin 33))
      (node (ref U1) (pin 4)))
    (net (code 34) (name /SMI_SD0)
      (node (ref J3) (pin 24))
      (node (ref U2) (pin 7)))
    (net (code 35) (name /SMI_SD3)
      (node (ref J3) (pin 23))
      (node (ref U1) (pin 5)))
    (net (code 36) (name /SMI_SD17)
      (node (ref U2) (pin 6))
      (node (ref J3) (pin 22)))
    (net (code 37) (name /SMI_SD1)
      (node (ref J3) (pin 21))
      (node (ref U1) (pin 6)))
    (net (code 38) (name /SMI_SD2)
      (node (ref J3) (pin 19))
      (node (ref U1) (pin 7)))
    (net (code 39) (name /SMI_SD8)
      (node (ref J3) (pin 36))
      (node (ref U2) (pin 9)))
    (net (code 40) (name /SMI_SD13)
      (node (ref U1) (pin 2))
      (node (ref J3) (pin 40))
      (node (ref U1) (pin 3)))
    (net (code 41) (name /SMI_SD6)
      (node (ref J3) (pin 8))
      (node (ref U2) (pin 2)))
    (net (code 42) (name "Net-(J1-Pad5)")
      (node (ref J1) (pin 5)))
    (net (code 43) (name "Net-(J1-Pad3)")
      (node (ref J1) (pin 3)))
    (net (code 44) (name "Net-(J1-Pad2)")
      (node (ref J1) (pin 2)))
    (net (code 45) (name "Net-(R2-Pad1)")
      (node (ref U2) (pin 1))
      (node (ref R2) (pin 1)))
    (net (code 46) (name "Net-(U2-Pad16)")
      (node (ref U2) (pin 16)))
    (net (code 47) (name "Net-(U2-Pad17)")
      (node (ref U2) (pin 17)))
    (net (code 48) (name "Net-(U2-Pad18)")
      (node (ref U2) (pin 18)))
    (net (code 49) (name "Net-(U2-Pad15)")
      (node (ref U2) (pin 15)))
    (net (code 50) (name "Net-(U2-Pad14)")
      (node (ref U2) (pin 14)))
    (net (code 51) (name "Net-(U2-Pad13)")
      (node (ref U2) (pin 13)))
    (net (code 52) (name "Net-(U2-Pad12)")
      (node (ref U2) (pin 12)))
    (net (code 53) (name "Net-(U2-Pad11)")
      (node (ref U2) (pin 11)))))